|  |  |  |
| --- | --- | --- |
|  | **Port** | **Address in PC** |
| **PPI** | Port A | **60 H** |
| Port B | **61 H** |
| Port C | **62 H** |
| Command Register | **63 H** |
| **PIT** | Counter 0 | **40 H** |
| Counter 1 | **41 H** |
| Counter 2 | **42 H** |
| Command Register | **43 H** |

***O 43 , B6 //*** to initialize the counter

***O 42 , E8***

***O 42 , 03 //*** send the count 03E8h to counter 2

***O 61 , 03 //*** to enable G2 (the speaker will start)

***O 61 , 00 //*** to disable G2 (the speaker will stop)