|  |  |  |
| --- | --- | --- |
|  |  **Port** |  **Address in PC** |
| **PPI** |  Port A |  **60 H** |
|  Port B |  **61 H** |
|  Port C |  **62 H** |
| Command Register |  **63 H** |
| **PIT** |  Counter 0 |  **40 H** |
|  Counter 1 |  **41 H** |
|  Counter 2 |  **42 H** |
| Command Register |  **43 H** |

 ***O 43 , B6 //*** to initialize the counter

 ***O 42 , E8***

 ***O 42 , 03 //*** send the count 03E8h to counter 2

 ***O 61 , 03 //*** to enable G2 (the speaker will start)

 ***O 61 , 00 //*** to disable G2 (the speaker will stop)