

**Birzeit University**

**Faculty of Engineering & Techonology**

**Department of Electrical & Computer Engineering**

**ENEE**

**“Prelab Exp#7”**

**Student :Mohamad Bornat #1130842**

**Instructor: Dr.Jasser Sa’ed**

**Date: 18\7\2016**

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  |  |

1. Rth=Rint , Vdc=Vth

P = I2 \* RL = ()2 \* RL

To find maximum power transfer, take the partial derivative with respect to RL:-

P is maximized when derivative =0 .

**So RL=Rth**

Rl = 30 ohm

Pmax = ()2 \* RL = ()2 \* 30 = 0.208 W

2.to find max power, let’s find Rth ,Vth.

Rth={[(1.2k//2.2k)+390]//820 }+680

Vth, open the RL .

I=15/Req , Req=1980.4ohm


Itotal= 7.5mA

Current divider

I(through 820ohm)=2200\*7.5m/(390+2200+820) = 4.88mA

Vth=820\*5.5m=4V

Pmax=Vth^2 /(4\*Rth) = 3.456mWatt



The max cursor point refers to (1.161k,3.4550m).



4.

1 and 2



3-Pf=Cos (

Qc=-Qi …..total reactive power absorbed must equal zero since pf is unity .

X=

C