

Department Of electrical and computer Engineering

ENEE2103 CIRCUITS AND ELECTRONICS LABORATORY

Experiment No.9 Prelab

Insructer: Dr. Alhareth Zyoud

Made By: Islam Jihad

ID: 1191375

TA: MR. Ismail Abualia

Date: 7/Nov/2021

***I.ZENER DIODE.***

Part1:





Part2:





Part3:



With dc sweep and Vin=0



Vdc=10V and sweep the resistance





***II. THE VOLTAGE REGULATED POWER SUPPLY.***



VOUT=9.33V

V­IN=15V

V­­­Z=4.665V

V­OUT= 2\*V­Z

When I added the load resister to the output the output was=9.3295V

And the current output was=9.33mA

3.

A. for R=680 I got the same voltage for r=1k but the current was =13.72mA

B. for R=470 I got the same voltage for r=1k but the current was =19.85mA

C. for R=220 I got the same voltage for r=1k but the current was =42.41mA

D. for R=100 the PSpice can’t solve it due to low resistance

4. I got the same error for small values



But I think it will be bigger, Vout> Vz

5. when R2=2.2k the output voltage were= 6.7851V



7. I got the same error because of the 10ohm resister and I can’t calculate anything

8. the 10 ohm resister prevent me from calculating or adding any other component

