# -------------------------------------------------------------------------- #
#
# Copyright (C) 1991-2009 Altera Corporation
# Your use of Altera Corporation's design tools, logic functions 
# and other software and tools, and its AMPP partner logic 
# functions, and any output files from any of the foregoing 
# (including device programming or simulation files), and any 
# associated documentation or information are expressly subject 
# to the terms and conditions of the Altera Program License 
# Subscription Agreement, Altera MegaCore Function License 
# Agreement, or other applicable license agreement, including, 
# without limitation, that your use is for the sole purpose of 
# programming logic devices manufactured by Altera and sold by 
# Altera or its authorized distributors.  Please refer to the 
# applicable agreement for further details.
#
# -------------------------------------------------------------------------- #
#
# Quartus II
# Version 9.0 Build 132 02/25/2009 SJ Web Edition
# Date created = 23:03:32  March 30, 2010
#
# -------------------------------------------------------------------------- #
#
# Notes:
#
# 1) The default values for assignments are stored in the file:
#		SecuritySystem_assignment_defaults.qdf
#    If this file doesn't exist, see file:
#		assignment_defaults.qdf
#
# 2) Altera recommends that you do not modify this file. This
#    file is updated automatically by the Quartus II software
#    and any changes you make may be lost or overwritten.
#
# -------------------------------------------------------------------------- #


set_global_assignment -name FAMILY "Cyclone II"
set_global_assignment -name DEVICE EP2C20F484C7
set_global_assignment -name TOP_LEVEL_ENTITY SecuritySystem
set_global_assignment -name ORIGINAL_QUARTUS_VERSION 9.0
set_global_assignment -name PROJECT_CREATION_TIME_DATE "23:03:32  MARCH 30, 2010"
set_global_assignment -name LAST_QUARTUS_VERSION 9.0
set_global_assignment -name USE_GENERATED_PHYSICAL_CONSTRAINTS OFF -section_id eda_blast_fpga
set_global_assignment -name MIN_CORE_JUNCTION_TEMP 0
set_global_assignment -name MAX_CORE_JUNCTION_TEMP 85
set_global_assignment -name BDF_FILE SecuritySystem.bdf
set_instance_assignment -name PARTITION_HIERARCHY root_partition -to | -section_id Top
set_global_assignment -name PARTITION_NETLIST_TYPE SOURCE -section_id Top
set_global_assignment -name PARTITION_COLOR 16764057 -section_id Top
set_global_assignment -name LL_ROOT_REGION ON -section_id "Root Region"
set_global_assignment -name LL_MEMBER_STATE LOCKED -section_id "Root Region"
set_global_assignment -name SIMULATION_MODE FUNCTIONAL
set_global_assignment -name VECTOR_WAVEFORM_FILE SecuritySystem.vwf
set_location_assignment PIN_D12 -to CLK
set_location_assignment PIN_L22 -to en
set_location_assignment PIN_L21 -to Sel[0]
set_location_assignment PIN_M22 -to Sel[1]
set_location_assignment PIN_V12 -to I0
set_location_assignment PIN_W12 -to I1
set_location_assignment PIN_U12 -to I2
set_location_assignment PIN_U11 -to I3
set_location_assignment PIN_M2 -to I4
set_location_assignment PIN_M1 -to I5
set_location_assignment PIN_L2 -to I6
set_location_assignment PIN_J2 -to Dis1[0]
set_location_assignment PIN_J1 -to Dis1[1]
set_location_assignment PIN_H2 -to Dis1[2]
set_location_assignment PIN_H1 -to Dis1[3]
set_location_assignment PIN_F2 -to Dis1[4]
set_location_assignment PIN_F1 -to Dis1[5]
set_location_assignment PIN_E2 -to Dis1[6]
set_location_assignment PIN_E1 -to Dis2[0]
set_location_assignment PIN_H6 -to Dis2[1]
set_location_assignment PIN_H5 -to Dis2[2]
set_location_assignment PIN_H4 -to Dis2[3]
set_location_assignment PIN_G3 -to Dis2[4]
set_location_assignment PIN_D2 -to Dis2[5]
set_location_assignment PIN_D1 -to Dis2[6]
set_location_assignment PIN_G5 -to Dis3[0]
set_location_assignment PIN_G6 -to Dis3[1]
set_location_assignment PIN_C2 -to Dis3[2]
set_location_assignment PIN_C1 -to Dis3[3]
set_location_assignment PIN_E3 -to Dis3[4]
set_location_assignment PIN_E4 -to Dis3[5]
set_location_assignment PIN_D3 -to Dis3[6]
set_location_assignment PIN_F4 -to Dis4[0]
set_location_assignment PIN_D5 -to Dis4[1]
set_location_assignment PIN_D6 -to Dis4[2]
set_location_assignment PIN_J4 -to Dis4[3]
set_location_assignment PIN_L8 -to Dis4[4]
set_location_assignment PIN_F3 -to Dis4[5]
set_location_assignment PIN_D4 -to Dis4[6]
set_location_assignment PIN_R20 -to red
set_location_assignment PIN_U22 -to green