Version:
	9.0 Build 132 02/25/2009 SJ Web Edition

Chip Device Options:
	Device Name:	EP2C20F484C7
	Device JTAG code:	ffffffff
	Programming_mode:	Active Serial Configuration
	NWS_NRS_NCS:	UNRESERVED
	RDYNBUSY:	UNRESERVED
	DATA 7 to 1:	UNRESERVED
	nCEO:	RESERVED_GND
	UNUSED PINS:	RESERVED_GND
	Default IO Standard::	3.3-V LVTTL
	User Start-up Clock:	0
	Auto Restart on Error:	1
	Release Clears Before Tristates:	0
	Device Clear:	0
	Test And Scan:	0
	Device OE:	0
	Enable Lock Output:	0
	Enable Init Done:	0
	Enable JTAG BST:	0
	Enable Vref A:	0
	Enable Vref B:	0



****************************
******Individual Atoms******
****************************

- ATOM ------------------------
	ATOM_NAME: inst5 -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 5
	Atom Type: cycloneii_lcell_comb

	INPUTS (Driven By):
		0: [DATAA]	  C	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:CONNECTED,NONE
		1: [DATAB]	  B	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:CONNECTED,NONE
		2: [DATAC]	  D	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:CONNECTED,NONE
		3: [DATAD]	  A	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:CONNECTED,NONE
		4: NO ITERM
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	inst5	LIT INDEX 0 FANOUTS 1
		1: NONE

	PARAMETER LIST:
		sum_lutc_input                 = datac
		lut_mask                       = 88f0


- ATOM ------------------------
	ATOM_NAME: F -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 8
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  inst5	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	F	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: C -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 9
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: NO ITERM
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: [PADIO]	DISCONNECTED
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	C	LIT INDEX 0 FANOUTS 1
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	C	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = input
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	0
		PAD TO CORE 1:	0
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: B -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 10
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: NO ITERM
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: [PADIO]	DISCONNECTED
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	B	LIT INDEX 0 FANOUTS 1
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	B	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = input
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	0
		PAD TO CORE 1:	0
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: D -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 11
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: NO ITERM
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: [PADIO]	DISCONNECTED
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	D	LIT INDEX 0 FANOUTS 1
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	D	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = input
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	0
		PAD TO CORE 1:	0
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: A -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 12
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: NO ITERM
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: [PADIO]	DISCONNECTED
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	A	LIT INDEX 0 FANOUTS 1
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	A	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = input
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	0
		PAD TO CORE 1:	0
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: ~QUARTUS_CREATED_GND~I -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 13
	Atom Type: cycloneii_lcell_comb

	INPUTS (Driven By):
		0: NO ITERM
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	~QUARTUS_CREATED_GND~I	LIT INDEX 0 FANOUTS 0
		1: NONE

	PARAMETER LIST:
		(Skipping parameters for lcell or lcell comb with no fanout)


- ATOM ------------------------
	ATOM_NAME: ~ASDO~ -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 14
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: NO ITERM
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	~ASDO~	LIT INDEX 0 FANOUTS 0
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	~ASDO~	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = input
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	0
		PAD TO CORE 1:	0
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		OFF

- ATOM ------------------------
	ATOM_NAME: ~nCSO~ -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 15
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: NO ITERM
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	~nCSO~	LIT INDEX 0 FANOUTS 0
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	~nCSO~	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = input
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	0
		PAD TO CORE 1:	0
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		OFF

- ATOM ------------------------
	ATOM_NAME: ~LVDS91p/nCEO~ -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 16
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  GND	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	~LVDS91p/nCEO~	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

