Version:
	9.0 Build 132 02/25/2009 SJ Web Edition

Chip Device Options:
	Device Name:	EP2C20F484C7
	Device JTAG code:	ffffffff
	Programming_mode:	Active Serial Configuration
	NWS_NRS_NCS:	UNRESERVED
	RDYNBUSY:	UNRESERVED
	DATA 7 to 1:	UNRESERVED
	nCEO:	RESERVED_GND
	UNUSED PINS:	RESERVED_GND
	Default IO Standard::	3.3-V LVTTL
	User Start-up Clock:	0
	Auto Restart on Error:	1
	Release Clears Before Tristates:	0
	Device Clear:	0
	Test And Scan:	0
	Device OE:	0
	Enable Lock Output:	0
	Enable Init Done:	0
	Enable JTAG BST:	0
	Enable Vref A:	0
	Enable Vref B:	0



****************************
******Individual Atoms******
****************************

- ATOM ------------------------
	ATOM_NAME: MyMemory:inst|MyDFF:inst10|Q -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 32
	Atom Type: cycloneii_lcell_ff

	power up = low

	INPUTS (Driven By):
		0: [CLK]	  CLK	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAIN]	  MyDriver:inst17|WideOr1~2	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: [ENA]	  MyDecoder:inst8|out[3]~4	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
	OUTPUTS (Int. Connections):
		0: [REGOUT]	MyMemory:inst|MyDFF:inst10|Q	LIT INDEX 0 FANOUTS 2 REGED POS

	PARAMETER LIST:
		EMPTY!!


- ATOM ------------------------
	ATOM_NAME: MyMemory:inst|MyDFF:inst13|Q -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 33
	Atom Type: cycloneii_lcell_ff

	power up = low

	INPUTS (Driven By):
		0: [CLK]	  CLK	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAIN]	  MyDriver:inst17|out_v[5]~2	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: [ENA]	  MyDecoder:inst8|out[3]~4	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
	OUTPUTS (Int. Connections):
		0: [REGOUT]	MyMemory:inst|MyDFF:inst13|Q	LIT INDEX 0 FANOUTS 2 REGED POS

	PARAMETER LIST:
		EMPTY!!


- ATOM ------------------------
	ATOM_NAME: MyMemory:inst|MyDFF:inst14|Q -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 34
	Atom Type: cycloneii_lcell_ff

	power up = low

	INPUTS (Driven By):
		0: [CLK]	  CLK	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAIN]	  MyDriver:inst17|out_v[6]~3	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: [ENA]	  MyDecoder:inst8|out[3]~4	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
	OUTPUTS (Int. Connections):
		0: [REGOUT]	MyMemory:inst|MyDFF:inst14|Q	LIT INDEX 0 FANOUTS 3 REGED POS

	PARAMETER LIST:
		EMPTY!!


- ATOM ------------------------
	ATOM_NAME: MyMemory:inst|MyDFF:inst12|Q -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 35
	Atom Type: cycloneii_lcell_ff

	power up = low

	INPUTS (Driven By):
		0: [CLK]	  CLK	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAIN]	  MyDriver:inst17|Decoder0~0	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: [ENA]	  MyDecoder:inst8|out[3]~4	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
	OUTPUTS (Int. Connections):
		0: [REGOUT]	MyMemory:inst|MyDFF:inst12|Q	LIT INDEX 0 FANOUTS 2 REGED POS

	PARAMETER LIST:
		EMPTY!!


- ATOM ------------------------
	ATOM_NAME: inst21~0 -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 36
	Atom Type: cycloneii_lcell_comb

	INPUTS (Driven By):
		0: [DATAA]	  MyMemory:inst|MyDFF:inst10|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAB]	  MyMemory:inst|MyDFF:inst13|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: [DATAC]	  MyMemory:inst|MyDFF:inst14|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		3: [DATAD]	  MyMemory:inst|MyDFF:inst12|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		4: NO ITERM
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	inst21~0	LIT INDEX 0 FANOUTS 1
		1: NONE

	PARAMETER LIST:
		sum_lutc_input                 = datac
		lut_mask                       = 0008


- ATOM ------------------------
	ATOM_NAME: MyMemory:inst|MyDFF:inst9|Q -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 37
	Atom Type: cycloneii_lcell_ff

	power up = low

	INPUTS (Driven By):
		0: [CLK]	  CLK	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAIN]	  MyDriver:inst17|WideOr2~0	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: [ENA]	  MyDecoder:inst8|out[3]~4	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
	OUTPUTS (Int. Connections):
		0: [REGOUT]	MyMemory:inst|MyDFF:inst9|Q	LIT INDEX 0 FANOUTS 2 REGED POS

	PARAMETER LIST:
		EMPTY!!


- ATOM ------------------------
	ATOM_NAME: MyMemory:inst|MyDFF:inst8|Q -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 38
	Atom Type: cycloneii_lcell_ff

	power up = low

	INPUTS (Driven By):
		0: [CLK]	  CLK	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAIN]	  MyDriver:inst17|WideOr3~4	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: [ENA]	  MyDecoder:inst8|out[3]~4	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
	OUTPUTS (Int. Connections):
		0: [REGOUT]	MyMemory:inst|MyDFF:inst8|Q	LIT INDEX 0 FANOUTS 2 REGED POS

	PARAMETER LIST:
		EMPTY!!


- ATOM ------------------------
	ATOM_NAME: MyMemory:inst24|MyDFF:inst10|Q -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 39
	Atom Type: cycloneii_lcell_ff

	power up = low

	INPUTS (Driven By):
		0: [CLK]	  CLK	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAIN]	  MyDriver:inst17|WideOr1~2	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: [ENA]	  MyDecoder:inst8|out[2]~5	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
	OUTPUTS (Int. Connections):
		0: [REGOUT]	MyMemory:inst24|MyDFF:inst10|Q	LIT INDEX 0 FANOUTS 2 REGED POS

	PARAMETER LIST:
		EMPTY!!


- ATOM ------------------------
	ATOM_NAME: MyMemory:inst24|MyDFF:inst14|Q -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 40
	Atom Type: cycloneii_lcell_ff

	power up = low

	INPUTS (Driven By):
		0: [CLK]	  CLK	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAIN]	  MyDriver:inst17|out_v[6]~3	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: [ENA]	  MyDecoder:inst8|out[2]~5	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
	OUTPUTS (Int. Connections):
		0: [REGOUT]	MyMemory:inst24|MyDFF:inst14|Q	LIT INDEX 0 FANOUTS 3 REGED POS

	PARAMETER LIST:
		EMPTY!!


- ATOM ------------------------
	ATOM_NAME: inst21~1 -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 41
	Atom Type: cycloneii_lcell_comb

	INPUTS (Driven By):
		0: [DATAA]	  MyMemory:inst|MyDFF:inst9|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAB]	  MyMemory:inst|MyDFF:inst8|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: [DATAC]	  MyMemory:inst24|MyDFF:inst10|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		3: [DATAD]	  MyMemory:inst24|MyDFF:inst14|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		4: NO ITERM
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	inst21~1	LIT INDEX 0 FANOUTS 1
		1: NONE

	PARAMETER LIST:
		sum_lutc_input                 = datac
		lut_mask                       = 0001


- ATOM ------------------------
	ATOM_NAME: MyMemory:inst24|MyDFF:inst13|Q -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 42
	Atom Type: cycloneii_lcell_ff

	power up = low

	INPUTS (Driven By):
		0: [CLK]	  CLK	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAIN]	  MyDriver:inst17|out_v[5]~2	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: [ENA]	  MyDecoder:inst8|out[2]~5	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
	OUTPUTS (Int. Connections):
		0: [REGOUT]	MyMemory:inst24|MyDFF:inst13|Q	LIT INDEX 0 FANOUTS 2 REGED POS

	PARAMETER LIST:
		EMPTY!!


- ATOM ------------------------
	ATOM_NAME: MyMemory:inst24|MyDFF:inst12|Q -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 43
	Atom Type: cycloneii_lcell_ff

	power up = low

	INPUTS (Driven By):
		0: [CLK]	  CLK	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAIN]	  MyDriver:inst17|Decoder0~0	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: [ENA]	  MyDecoder:inst8|out[2]~5	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
	OUTPUTS (Int. Connections):
		0: [REGOUT]	MyMemory:inst24|MyDFF:inst12|Q	LIT INDEX 0 FANOUTS 2 REGED POS

	PARAMETER LIST:
		EMPTY!!


- ATOM ------------------------
	ATOM_NAME: MyMemory:inst24|MyDFF:inst9|Q -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 44
	Atom Type: cycloneii_lcell_ff

	power up = low

	INPUTS (Driven By):
		0: [CLK]	  CLK	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAIN]	  MyDriver:inst17|WideOr2~0	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: [ENA]	  MyDecoder:inst8|out[2]~5	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
	OUTPUTS (Int. Connections):
		0: [REGOUT]	MyMemory:inst24|MyDFF:inst9|Q	LIT INDEX 0 FANOUTS 2 REGED POS

	PARAMETER LIST:
		EMPTY!!


- ATOM ------------------------
	ATOM_NAME: MyMemory:inst24|MyDFF:inst8|Q -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 45
	Atom Type: cycloneii_lcell_ff

	power up = low

	INPUTS (Driven By):
		0: [CLK]	  CLK	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAIN]	  MyDriver:inst17|WideOr3~4	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: [ENA]	  MyDecoder:inst8|out[2]~5	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
	OUTPUTS (Int. Connections):
		0: [REGOUT]	MyMemory:inst24|MyDFF:inst8|Q	LIT INDEX 0 FANOUTS 2 REGED POS

	PARAMETER LIST:
		EMPTY!!


- ATOM ------------------------
	ATOM_NAME: inst21~2 -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 46
	Atom Type: cycloneii_lcell_comb

	INPUTS (Driven By):
		0: [DATAA]	  MyMemory:inst24|MyDFF:inst13|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAB]	  MyMemory:inst24|MyDFF:inst12|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: [DATAC]	  MyMemory:inst24|MyDFF:inst9|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		3: [DATAD]	  MyMemory:inst24|MyDFF:inst8|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		4: NO ITERM
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	inst21~2	LIT INDEX 0 FANOUTS 1
		1: NONE

	PARAMETER LIST:
		sum_lutc_input                 = datac
		lut_mask                       = 0002


- ATOM ------------------------
	ATOM_NAME: MyMemory:inst25|MyDFF:inst10|Q -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 47
	Atom Type: cycloneii_lcell_ff

	power up = low

	INPUTS (Driven By):
		0: [CLK]	  CLK	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAIN]	  MyDriver:inst17|WideOr1~2	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: [ENA]	  MyDecoder:inst8|out[1]~6	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
	OUTPUTS (Int. Connections):
		0: [REGOUT]	MyMemory:inst25|MyDFF:inst10|Q	LIT INDEX 0 FANOUTS 2 REGED POS

	PARAMETER LIST:
		EMPTY!!


- ATOM ------------------------
	ATOM_NAME: MyMemory:inst25|MyDFF:inst13|Q -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 48
	Atom Type: cycloneii_lcell_ff

	power up = low

	INPUTS (Driven By):
		0: [CLK]	  CLK	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAIN]	  MyDriver:inst17|out_v[5]~2	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: [ENA]	  MyDecoder:inst8|out[1]~6	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
	OUTPUTS (Int. Connections):
		0: [REGOUT]	MyMemory:inst25|MyDFF:inst13|Q	LIT INDEX 0 FANOUTS 2 REGED POS

	PARAMETER LIST:
		EMPTY!!


- ATOM ------------------------
	ATOM_NAME: MyMemory:inst25|MyDFF:inst14|Q -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 49
	Atom Type: cycloneii_lcell_ff

	power up = low

	INPUTS (Driven By):
		0: [CLK]	  CLK	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAIN]	  MyDriver:inst17|out_v[6]~3	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: [ENA]	  MyDecoder:inst8|out[1]~6	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
	OUTPUTS (Int. Connections):
		0: [REGOUT]	MyMemory:inst25|MyDFF:inst14|Q	LIT INDEX 0 FANOUTS 3 REGED POS

	PARAMETER LIST:
		EMPTY!!


- ATOM ------------------------
	ATOM_NAME: MyMemory:inst25|MyDFF:inst12|Q -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 50
	Atom Type: cycloneii_lcell_ff

	power up = low

	INPUTS (Driven By):
		0: [CLK]	  CLK	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAIN]	  MyDriver:inst17|Decoder0~0	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: [ENA]	  MyDecoder:inst8|out[1]~6	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
	OUTPUTS (Int. Connections):
		0: [REGOUT]	MyMemory:inst25|MyDFF:inst12|Q	LIT INDEX 0 FANOUTS 2 REGED POS

	PARAMETER LIST:
		EMPTY!!


- ATOM ------------------------
	ATOM_NAME: inst21~3 -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 51
	Atom Type: cycloneii_lcell_comb

	INPUTS (Driven By):
		0: [DATAA]	  MyMemory:inst25|MyDFF:inst10|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAB]	  MyMemory:inst25|MyDFF:inst13|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: [DATAC]	  MyMemory:inst25|MyDFF:inst14|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		3: [DATAD]	  MyMemory:inst25|MyDFF:inst12|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		4: NO ITERM
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	inst21~3	LIT INDEX 0 FANOUTS 1
		1: NONE

	PARAMETER LIST:
		sum_lutc_input                 = datac
		lut_mask                       = 0008


- ATOM ------------------------
	ATOM_NAME: inst21~4 -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 52
	Atom Type: cycloneii_lcell_comb

	INPUTS (Driven By):
		0: [DATAA]	  inst21~0	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAB]	  inst21~1	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: [DATAC]	  inst21~2	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		3: [DATAD]	  inst21~3	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		4: NO ITERM
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	inst21~4	LIT INDEX 0 FANOUTS 1
		1: NONE

	PARAMETER LIST:
		sum_lutc_input                 = datac
		lut_mask                       = 8000


- ATOM ------------------------
	ATOM_NAME: MyMemory:inst25|MyDFF:inst9|Q -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 53
	Atom Type: cycloneii_lcell_ff

	power up = low

	INPUTS (Driven By):
		0: [CLK]	  CLK	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAIN]	  MyDriver:inst17|WideOr2~0	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: [ENA]	  MyDecoder:inst8|out[1]~6	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
	OUTPUTS (Int. Connections):
		0: [REGOUT]	MyMemory:inst25|MyDFF:inst9|Q	LIT INDEX 0 FANOUTS 2 REGED POS

	PARAMETER LIST:
		EMPTY!!


- ATOM ------------------------
	ATOM_NAME: MyMemory:inst25|MyDFF:inst8|Q -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 54
	Atom Type: cycloneii_lcell_ff

	power up = low

	INPUTS (Driven By):
		0: [CLK]	  CLK	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAIN]	  MyDriver:inst17|WideOr3~4	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: [ENA]	  MyDecoder:inst8|out[1]~6	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
	OUTPUTS (Int. Connections):
		0: [REGOUT]	MyMemory:inst25|MyDFF:inst8|Q	LIT INDEX 0 FANOUTS 2 REGED POS

	PARAMETER LIST:
		EMPTY!!


- ATOM ------------------------
	ATOM_NAME: MyMemory:inst26|MyDFF:inst10|Q -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 55
	Atom Type: cycloneii_lcell_ff

	power up = low

	INPUTS (Driven By):
		0: [CLK]	  CLK	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAIN]	  MyDriver:inst17|WideOr1~2	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: [ENA]	  MyDecoder:inst8|out[0]~7	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
	OUTPUTS (Int. Connections):
		0: [REGOUT]	MyMemory:inst26|MyDFF:inst10|Q	LIT INDEX 0 FANOUTS 2 REGED POS

	PARAMETER LIST:
		EMPTY!!


- ATOM ------------------------
	ATOM_NAME: MyMemory:inst26|MyDFF:inst14|Q -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 56
	Atom Type: cycloneii_lcell_ff

	power up = low

	INPUTS (Driven By):
		0: [CLK]	  CLK	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAIN]	  MyDriver:inst17|out_v[6]~3	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: [ENA]	  MyDecoder:inst8|out[0]~7	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
	OUTPUTS (Int. Connections):
		0: [REGOUT]	MyMemory:inst26|MyDFF:inst14|Q	LIT INDEX 0 FANOUTS 3 REGED POS

	PARAMETER LIST:
		EMPTY!!


- ATOM ------------------------
	ATOM_NAME: inst21~5 -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 57
	Atom Type: cycloneii_lcell_comb

	INPUTS (Driven By):
		0: [DATAA]	  MyMemory:inst25|MyDFF:inst9|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAB]	  MyMemory:inst25|MyDFF:inst8|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: [DATAC]	  MyMemory:inst26|MyDFF:inst10|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		3: [DATAD]	  MyMemory:inst26|MyDFF:inst14|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		4: NO ITERM
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	inst21~5	LIT INDEX 0 FANOUTS 1
		1: NONE

	PARAMETER LIST:
		sum_lutc_input                 = datac
		lut_mask                       = 0001


- ATOM ------------------------
	ATOM_NAME: MyMemory:inst26|MyDFF:inst13|Q -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 58
	Atom Type: cycloneii_lcell_ff

	power up = low

	INPUTS (Driven By):
		0: [CLK]	  CLK	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAIN]	  MyDriver:inst17|out_v[5]~2	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: [ENA]	  MyDecoder:inst8|out[0]~7	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
	OUTPUTS (Int. Connections):
		0: [REGOUT]	MyMemory:inst26|MyDFF:inst13|Q	LIT INDEX 0 FANOUTS 2 REGED POS

	PARAMETER LIST:
		EMPTY!!


- ATOM ------------------------
	ATOM_NAME: MyMemory:inst26|MyDFF:inst12|Q -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 59
	Atom Type: cycloneii_lcell_ff

	power up = low

	INPUTS (Driven By):
		0: [CLK]	  CLK	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAIN]	  MyDriver:inst17|Decoder0~0	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: [ENA]	  MyDecoder:inst8|out[0]~7	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
	OUTPUTS (Int. Connections):
		0: [REGOUT]	MyMemory:inst26|MyDFF:inst12|Q	LIT INDEX 0 FANOUTS 2 REGED POS

	PARAMETER LIST:
		EMPTY!!


- ATOM ------------------------
	ATOM_NAME: MyMemory:inst26|MyDFF:inst9|Q -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 60
	Atom Type: cycloneii_lcell_ff

	power up = low

	INPUTS (Driven By):
		0: [CLK]	  CLK	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAIN]	  MyDriver:inst17|WideOr2~0	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: [ENA]	  MyDecoder:inst8|out[0]~7	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
	OUTPUTS (Int. Connections):
		0: [REGOUT]	MyMemory:inst26|MyDFF:inst9|Q	LIT INDEX 0 FANOUTS 2 REGED POS

	PARAMETER LIST:
		EMPTY!!


- ATOM ------------------------
	ATOM_NAME: MyMemory:inst26|MyDFF:inst8|Q -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 61
	Atom Type: cycloneii_lcell_ff

	power up = low

	INPUTS (Driven By):
		0: [CLK]	  CLK	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAIN]	  MyDriver:inst17|WideOr3~4	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: [ENA]	  MyDecoder:inst8|out[0]~7	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
	OUTPUTS (Int. Connections):
		0: [REGOUT]	MyMemory:inst26|MyDFF:inst8|Q	LIT INDEX 0 FANOUTS 2 REGED POS

	PARAMETER LIST:
		EMPTY!!


- ATOM ------------------------
	ATOM_NAME: inst21~6 -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 62
	Atom Type: cycloneii_lcell_comb

	INPUTS (Driven By):
		0: [DATAA]	  MyMemory:inst26|MyDFF:inst13|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAB]	  MyMemory:inst26|MyDFF:inst12|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: [DATAC]	  MyMemory:inst26|MyDFF:inst9|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		3: [DATAD]	  MyMemory:inst26|MyDFF:inst8|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		4: NO ITERM
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	inst21~6	LIT INDEX 0 FANOUTS 1
		1: NONE

	PARAMETER LIST:
		sum_lutc_input                 = datac
		lut_mask                       = 0002


- ATOM ------------------------
	ATOM_NAME: inst21 -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 63
	Atom Type: cycloneii_lcell_comb

	INPUTS (Driven By):
		0: [DATAA]	  inst21~4	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAB]	  inst21~5	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: [DATAC]	  inst21~6	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		3: NO ITERM
		4: NO ITERM
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	inst21	LIT INDEX 0 FANOUTS 2
		1: NONE

	PARAMETER LIST:
		sum_lutc_input                 = datac
		lut_mask                       = 8080


- ATOM ------------------------
	ATOM_NAME: MYEncoder:inst10|en_out[0]~11 -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 67
	Atom Type: cycloneii_lcell_comb

	INPUTS (Driven By):
		0: [DATAA]	  i1	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: [DATAD]	  i2	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		4: NO ITERM
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	MYEncoder:inst10|en_out[0]~11	LIT INDEX 0 FANOUTS 1
		1: NONE

	PARAMETER LIST:
		sum_lutc_input                 = datac
		lut_mask                       = 00aa


- ATOM ------------------------
	ATOM_NAME: MYEncoder:inst10|en_out[0]~12 -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 70
	Atom Type: cycloneii_lcell_comb

	INPUTS (Driven By):
		0: [DATAA]	  i5	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAB]	  MYEncoder:inst10|en_out[0]~11	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: [DATAC]	  i3	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		3: [DATAD]	  i4	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		4: NO ITERM
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	MYEncoder:inst10|en_out[0]~12	LIT INDEX 0 FANOUTS 4
		1: NONE

	PARAMETER LIST:
		sum_lutc_input                 = datac
		lut_mask                       = aafe


- ATOM ------------------------
	ATOM_NAME: MYEncoder:inst10|en_out~13 -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 71
	Atom Type: cycloneii_lcell_comb

	INPUTS (Driven By):
		0: NO ITERM
		1: NO ITERM
		2: [DATAC]	  i4	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		3: [DATAD]	  i5	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		4: NO ITERM
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	MYEncoder:inst10|en_out~13	LIT INDEX 0 FANOUTS 4
		1: NONE

	PARAMETER LIST:
		sum_lutc_input                 = datac
		lut_mask                       = 000f


- ATOM ------------------------
	ATOM_NAME: MyDecoder:inst8|out[3]~4 -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 77
	Atom Type: cycloneii_lcell_comb

	INPUTS (Driven By):
		0: [DATAA]	  SEL[1]	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAB]	  EN	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: [DATAC]	  SEL[0]	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		3: NO ITERM
		4: NO ITERM
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	MyDecoder:inst8|out[3]~4	LIT INDEX 0 FANOUTS 6
		1: NONE

	PARAMETER LIST:
		sum_lutc_input                 = datac
		lut_mask                       = 8080


- ATOM ------------------------
	ATOM_NAME: MyDriver:inst17|out_v[5]~2 -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 78
	Atom Type: cycloneii_lcell_comb

	INPUTS (Driven By):
		0: [DATAA]	  i6	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAB]	  i5	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	MyDriver:inst17|out_v[5]~2	LIT INDEX 0 FANOUTS 4
		1: NONE

	PARAMETER LIST:
		sum_lutc_input                 = datac
		lut_mask                       = eeee


- ATOM ------------------------
	ATOM_NAME: MYEncoder:inst10|en_out~14 -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 79
	Atom Type: cycloneii_lcell_comb

	INPUTS (Driven By):
		0: [DATAA]	  i2	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAB]	  i3	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	MYEncoder:inst10|en_out~14	LIT INDEX 0 FANOUTS 3
		1: NONE

	PARAMETER LIST:
		sum_lutc_input                 = datac
		lut_mask                       = eeee


- ATOM ------------------------
	ATOM_NAME: MyDriver:inst17|out_v[6]~3 -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 80
	Atom Type: cycloneii_lcell_comb

	INPUTS (Driven By):
		0: [DATAA]	  MYEncoder:inst10|en_out[0]~12	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAB]	  MYEncoder:inst10|en_out~13	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: [DATAC]	  MYEncoder:inst10|en_out~14	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		3: [DATAD]	  i6	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		4: NO ITERM
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	MyDriver:inst17|out_v[6]~3	LIT INDEX 0 FANOUTS 4
		1: NONE

	PARAMETER LIST:
		sum_lutc_input                 = datac
		lut_mask                       = 0019


- ATOM ------------------------
	ATOM_NAME: MyDriver:inst17|Decoder0~0 -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 81
	Atom Type: cycloneii_lcell_comb

	INPUTS (Driven By):
		0: [DATAA]	  MYEncoder:inst10|en_out~13	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAB]	  MYEncoder:inst10|en_out~14	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: [DATAC]	  i6	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		3: [DATAD]	  MYEncoder:inst10|en_out[0]~12	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		4: NO ITERM
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	MyDriver:inst17|Decoder0~0	LIT INDEX 0 FANOUTS 4
		1: NONE

	PARAMETER LIST:
		sum_lutc_input                 = datac
		lut_mask                       = 0008


- ATOM ------------------------
	ATOM_NAME: MyDriver:inst17|WideOr2~0 -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 82
	Atom Type: cycloneii_lcell_comb

	INPUTS (Driven By):
		0: [DATAA]	  i6	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAB]	  MYEncoder:inst10|en_out[0]~12	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: [DATAC]	  MYEncoder:inst10|en_out~14	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		3: [DATAD]	  MYEncoder:inst10|en_out~13	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		4: NO ITERM
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	MyDriver:inst17|WideOr2~0	LIT INDEX 0 FANOUTS 4
		1: NONE

	PARAMETER LIST:
		sum_lutc_input                 = datac
		lut_mask                       = 5400


- ATOM ------------------------
	ATOM_NAME: MyDecoder:inst8|out[2]~5 -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 83
	Atom Type: cycloneii_lcell_comb

	INPUTS (Driven By):
		0: [DATAA]	  SEL[1]	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAB]	  EN	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: NO ITERM
		3: [DATAD]	  SEL[0]	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		4: NO ITERM
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	MyDecoder:inst8|out[2]~5	LIT INDEX 0 FANOUTS 6
		1: NONE

	PARAMETER LIST:
		sum_lutc_input                 = datac
		lut_mask                       = 0088


- ATOM ------------------------
	ATOM_NAME: MyDecoder:inst8|out[1]~6 -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 84
	Atom Type: cycloneii_lcell_comb

	INPUTS (Driven By):
		0: [DATAA]	  EN	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAB]	  SEL[0]	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: NO ITERM
		3: [DATAD]	  SEL[1]	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		4: NO ITERM
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	MyDecoder:inst8|out[1]~6	LIT INDEX 0 FANOUTS 6
		1: NONE

	PARAMETER LIST:
		sum_lutc_input                 = datac
		lut_mask                       = 0088


- ATOM ------------------------
	ATOM_NAME: MyDecoder:inst8|out[0]~7 -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 85
	Atom Type: cycloneii_lcell_comb

	INPUTS (Driven By):
		0: [DATAA]	  EN	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: [DATAC]	  SEL[1]	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		3: [DATAD]	  SEL[0]	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		4: NO ITERM
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	MyDecoder:inst8|out[0]~7	LIT INDEX 0 FANOUTS 6
		1: NONE

	PARAMETER LIST:
		sum_lutc_input                 = datac
		lut_mask                       = 000a


- ATOM ------------------------
	ATOM_NAME: MyDriver:inst17|WideOr1~2 -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 86
	Atom Type: cycloneii_lcell_comb

	INPUTS (Driven By):
		0: [DATAA]	  i4	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAB]	  i5	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: [DATAC]	  MYEncoder:inst10|en_out[0]~12	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		3: [DATAD]	  i6	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		4: NO ITERM
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	MyDriver:inst17|WideOr1~2	LIT INDEX 0 FANOUTS 4
		1: NONE

	PARAMETER LIST:
		sum_lutc_input                 = datac
		lut_mask                       = 00fe


- ATOM ------------------------
	ATOM_NAME: MyDriver:inst17|WideOr3~4 -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 87
	Atom Type: cycloneii_lcell_comb

	INPUTS (Driven By):
		0: [DATAA]	  i2	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: [DATAB]	  i3	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		2: [DATAC]	  i6	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		3: [DATAD]	  MYEncoder:inst10|en_out~13	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		4: NO ITERM
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	MyDriver:inst17|WideOr3~4	LIT INDEX 0 FANOUTS 4
		1: NONE

	PARAMETER LIST:
		sum_lutc_input                 = datac
		lut_mask                       = 0100


- ATOM ------------------------
	ATOM_NAME: red -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 97
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  !(inst21)	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	red	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: i0 -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 98
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: NO ITERM
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: [PADIO]	DISCONNECTED
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	i0	LIT INDEX 0 FANOUTS 0
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	i0	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = input
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	0
		PAD TO CORE 1:	0
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: dis -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 99
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: NO ITERM
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: [PADIO]	DISCONNECTED
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	dis	LIT INDEX 0 FANOUTS 0
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	dis	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = input
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	0
		PAD TO CORE 1:	0
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: green -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 100
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  inst21	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	green	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: DIS1[6] -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 101
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  MyMemory:inst26|MyDFF:inst8|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	DIS1[6]	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: DIS1[5] -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 102
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  MyMemory:inst26|MyDFF:inst9|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	DIS1[5]	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: DIS1[4] -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 103
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  MyMemory:inst26|MyDFF:inst10|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	DIS1[4]	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: DIS1[3] -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 104
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  MyMemory:inst26|MyDFF:inst14|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	DIS1[3]	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: DIS1[2] -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 105
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  MyMemory:inst26|MyDFF:inst12|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	DIS1[2]	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: DIS1[1] -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 106
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  MyMemory:inst26|MyDFF:inst13|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	DIS1[1]	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: DIS1[0] -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 107
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  MyMemory:inst26|MyDFF:inst14|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	DIS1[0]	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: DIS2[6] -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 108
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  MyMemory:inst25|MyDFF:inst8|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	DIS2[6]	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: DIS2[5] -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 109
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  MyMemory:inst25|MyDFF:inst9|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	DIS2[5]	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: DIS2[4] -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 110
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  MyMemory:inst25|MyDFF:inst10|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	DIS2[4]	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: DIS2[3] -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 111
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  MyMemory:inst25|MyDFF:inst14|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	DIS2[3]	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: DIS2[2] -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 112
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  MyMemory:inst25|MyDFF:inst12|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	DIS2[2]	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: DIS2[1] -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 113
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  MyMemory:inst25|MyDFF:inst13|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	DIS2[1]	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: DIS2[0] -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 114
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  MyMemory:inst25|MyDFF:inst14|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	DIS2[0]	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: DIS3[6] -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 115
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  MyMemory:inst24|MyDFF:inst8|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	DIS3[6]	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: DIS3[5] -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 116
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  MyMemory:inst24|MyDFF:inst9|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	DIS3[5]	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: DIS3[4] -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 117
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  MyMemory:inst24|MyDFF:inst10|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	DIS3[4]	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: DIS3[3] -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 118
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  MyMemory:inst24|MyDFF:inst14|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	DIS3[3]	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: DIS3[2] -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 119
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  MyMemory:inst24|MyDFF:inst12|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	DIS3[2]	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: DIS3[1] -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 120
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  MyMemory:inst24|MyDFF:inst13|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	DIS3[1]	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: DIS3[0] -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 121
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  MyMemory:inst24|MyDFF:inst14|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	DIS3[0]	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: DIS4[6] -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 122
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  MyMemory:inst|MyDFF:inst8|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	DIS4[6]	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: DIS4[5] -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 123
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  MyMemory:inst|MyDFF:inst9|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	DIS4[5]	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: DIS4[4] -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 124
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  MyMemory:inst|MyDFF:inst10|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	DIS4[4]	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: DIS4[3] -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 125
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  MyMemory:inst|MyDFF:inst14|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	DIS4[3]	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: DIS4[2] -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 126
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  MyMemory:inst|MyDFF:inst12|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	DIS4[2]	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: DIS4[1] -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 127
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  MyMemory:inst|MyDFF:inst13|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	DIS4[1]	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: DIS4[0] -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 128
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  MyMemory:inst|MyDFF:inst14|Q	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	DIS4[0]	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: i5 -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 129
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: NO ITERM
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: [PADIO]	DISCONNECTED
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	i5	LIT INDEX 0 FANOUTS 4
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	i5	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = input
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	0
		PAD TO CORE 1:	0
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: i1 -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 130
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: NO ITERM
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: [PADIO]	DISCONNECTED
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	i1	LIT INDEX 0 FANOUTS 1
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	i1	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = input
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	0
		PAD TO CORE 1:	0
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: i2 -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 131
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: NO ITERM
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: [PADIO]	DISCONNECTED
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	i2	LIT INDEX 0 FANOUTS 3
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	i2	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = input
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	0
		PAD TO CORE 1:	0
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: i3 -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 132
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: NO ITERM
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: [PADIO]	DISCONNECTED
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	i3	LIT INDEX 0 FANOUTS 3
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	i3	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = input
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	0
		PAD TO CORE 1:	0
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: i4 -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 133
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: NO ITERM
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: [PADIO]	DISCONNECTED
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	i4	LIT INDEX 0 FANOUTS 3
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	i4	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = input
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	0
		PAD TO CORE 1:	0
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: i6 -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 134
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: NO ITERM
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: [PADIO]	DISCONNECTED
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	i6	LIT INDEX 0 FANOUTS 6
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	i6	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = input
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	0
		PAD TO CORE 1:	0
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: CLK -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 135
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: NO ITERM
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: [PADIO]	DISCONNECTED
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	CLK	LIT INDEX 0 FANOUTS 24
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	CLK	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = input
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	0
		PAD TO CORE 1:	0
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: SEL[1] -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 136
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: NO ITERM
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: [PADIO]	DISCONNECTED
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	SEL[1]	LIT INDEX 0 FANOUTS 4
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	SEL[1]	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = input
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	0
		PAD TO CORE 1:	0
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: EN -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 137
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: NO ITERM
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: [PADIO]	DISCONNECTED
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	EN	LIT INDEX 0 FANOUTS 4
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	EN	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = input
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	0
		PAD TO CORE 1:	0
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: SEL[0] -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 138
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: NO ITERM
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: [PADIO]	DISCONNECTED
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	SEL[0]	LIT INDEX 0 FANOUTS 4
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	SEL[0]	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = input
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	0
		PAD TO CORE 1:	0
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

- ATOM ------------------------
	ATOM_NAME: ~QUARTUS_CREATED_GND~I -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 139
	Atom Type: cycloneii_lcell_comb

	INPUTS (Driven By):
		0: NO ITERM
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	~QUARTUS_CREATED_GND~I	LIT INDEX 0 FANOUTS 0
		1: NONE

	PARAMETER LIST:
		(Skipping parameters for lcell or lcell comb with no fanout)


- ATOM ------------------------
	ATOM_NAME: ~ASDO~ -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 140
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: NO ITERM
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	~ASDO~	LIT INDEX 0 FANOUTS 0
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	~ASDO~	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = input
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	0
		PAD TO CORE 1:	0
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		OFF

- ATOM ------------------------
	ATOM_NAME: ~nCSO~ -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 141
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: NO ITERM
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: [COMBOUT]	~nCSO~	LIT INDEX 0 FANOUTS 0
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	~nCSO~	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = input
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	0
		PAD TO CORE 1:	0
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		OFF

- ATOM ------------------------
	ATOM_NAME: ~LVDS91p/nCEO~ -- NON-UNIQUE
	Atom Hier Name: 
	Atom Id: 142
	Atom Type: cycloneii_io

	INPUTS (Driven By):
		0: [DATAIN]	  GND	LIT INDEX 0	GLOBAL:DONT_CARE	DELAY_CHAIN:UNCONNECTED
		1: NO ITERM
		2: NO ITERM
		3: NO ITERM
		4: NO ITERM
		5: NO ITERM
		6: NO ITERM
		7: NO ITERM
		8: NO ITERM
		9: NO ITERM
		10: NO ITERM
	OUTPUTS (Int. Connections):
		0: NONE
		1: NONE
		2: NONE
		3: NONE
		4: [PADIO]	~LVDS91p/nCEO~	LIT INDEX 0 FANOUTS 0
		5: NONE
		6: NONE

	PARAMETER LIST:
		operation_mode                 = output
		input_register_mode            = none
		output_register_mode           = none
		oe_register_mode               = none
		input_async_reset              = none
		output_async_reset             = none
		oe_async_reset                 = none
		input_sync_reset               = none
		output_sync_reset              = none
		oe_sync_reset                  = none
		input_power_up                 = low
		output_power_up                = low
		oe_power_up                    = low

	DELAY CHAINS:
		PAD TO CORE 0:	N/A
		PAD TO CORE 1:	N/A
		TCO CHAIN:	0
		TCOE CHAIN:	0
		PAD TO INPUT REG:	0

	IO STANDARD:			3.3-V LVTTL
	CURRENT STRENGTH:		DEFAULT
	PCI DIODE:       		OFF
	TERMINATION:     		OFF
	Output Duty Cycle:		BOTH_EDGES

