Classic Timing Analyzer report for all
Wed Mar 24 16:40:21 2010
Quartus II Version 9.0 Build 132 02/25/2009 SJ Web Edition


---------------------
; Table of Contents ;
---------------------
  1. Legal Notice
  2. Timing Analyzer Summary
  3. Timing Analyzer Settings
  4. Clock Settings Summary
  5. Parallel Compilation
  6. Clock Setup: 'clock'
  7. tsu
  8. tco
  9. th
 10. Timing Analyzer Messages



----------------
; Legal Notice ;
----------------
Copyright (C) 1991-2009 Altera Corporation
Your use of Altera Corporation's design tools, logic functions 
and other software and tools, and its AMPP partner logic 
functions, and any output files from any of the foregoing 
(including device programming or simulation files), and any 
associated documentation or information are expressly subject 
to the terms and conditions of the Altera Program License 
Subscription Agreement, Altera MegaCore Function License 
Agreement, or other applicable license agreement, including, 
without limitation, that your use is for the sole purpose of 
programming logic devices manufactured by Altera and sold by 
Altera or its authorized distributors.  Please refer to the 
applicable agreement for further details.



+----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; Timing Analyzer Summary                                                                                                                                                                ;
+------------------------------+-------+---------------+----------------------------------+--------------------------+----------------------------+------------+----------+--------------+
; Type                         ; Slack ; Required Time ; Actual Time                      ; From                     ; To                         ; From Clock ; To Clock ; Failed Paths ;
+------------------------------+-------+---------------+----------------------------------+--------------------------+----------------------------+------------+----------+--------------+
; Worst-case tsu               ; N/A   ; None          ; -2.654 ns                        ; reset                    ; counter:inst1|c[3]         ; --         ; clock    ; 0            ;
; Worst-case tco               ; N/A   ; None          ; 12.293 ns                        ; counter:inst1|c[1]       ; out[2]                     ; clock      ; --       ; 0            ;
; Worst-case th                ; N/A   ; None          ; 3.181 ns                         ; reset                    ; counter:inst1|c[0]         ; --         ; clock    ; 0            ;
; Clock Setup: 'clock'         ; N/A   ; None          ; 86.93 MHz ( period = 11.504 ns ) ; freq_div:inst|counter[7] ; freq_div:inst|counter[100] ; clock      ; clock    ; 0            ;
; Total number of failed paths ;       ;               ;                                  ;                          ;                            ;            ;          ; 0            ;
+------------------------------+-------+---------------+----------------------------------+--------------------------+----------------------------+------------+----------+--------------+


+--------------------------------------------------------------------------------------------------------------------+
; Timing Analyzer Settings                                                                                           ;
+---------------------------------------------------------------------+--------------------+------+----+-------------+
; Option                                                              ; Setting            ; From ; To ; Entity Name ;
+---------------------------------------------------------------------+--------------------+------+----+-------------+
; Device Name                                                         ; EP2C20F484C7       ;      ;    ;             ;
; Timing Models                                                       ; Final              ;      ;    ;             ;
; Default hold multicycle                                             ; Same as Multicycle ;      ;    ;             ;
; Cut paths between unrelated clock domains                           ; On                 ;      ;    ;             ;
; Cut off read during write signal paths                              ; On                 ;      ;    ;             ;
; Cut off feedback from I/O pins                                      ; On                 ;      ;    ;             ;
; Report Combined Fast/Slow Timing                                    ; Off                ;      ;    ;             ;
; Ignore Clock Settings                                               ; Off                ;      ;    ;             ;
; Analyze latches as synchronous elements                             ; On                 ;      ;    ;             ;
; Enable Recovery/Removal analysis                                    ; Off                ;      ;    ;             ;
; Enable Clock Latency                                                ; Off                ;      ;    ;             ;
; Use TimeQuest Timing Analyzer                                       ; Off                ;      ;    ;             ;
; Minimum Core Junction Temperature                                   ; 0                  ;      ;    ;             ;
; Maximum Core Junction Temperature                                   ; 85                 ;      ;    ;             ;
; Number of source nodes to report per destination node               ; 10                 ;      ;    ;             ;
; Number of destination nodes to report                               ; 10                 ;      ;    ;             ;
; Number of paths to report                                           ; 200                ;      ;    ;             ;
; Report Minimum Timing Checks                                        ; Off                ;      ;    ;             ;
; Use Fast Timing Models                                              ; Off                ;      ;    ;             ;
; Report IO Paths Separately                                          ; Off                ;      ;    ;             ;
; Perform Multicorner Analysis                                        ; On                 ;      ;    ;             ;
; Reports the worst-case path for each clock domain and analysis      ; Off                ;      ;    ;             ;
; Removes common clock path pessimism (CCPP) during slack computation ; Off                ;      ;    ;             ;
; Output I/O Timing Endpoint                                          ; Near End           ;      ;    ;             ;
+---------------------------------------------------------------------+--------------------+------+----+-------------+


+------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; Clock Settings Summary                                                                                                                                                             ;
+-----------------+--------------------+----------+------------------+---------------+--------------+----------+-----------------------+---------------------+--------+--------------+
; Clock Node Name ; Clock Setting Name ; Type     ; Fmax Requirement ; Early Latency ; Late Latency ; Based on ; Multiply Base Fmax by ; Divide Base Fmax by ; Offset ; Phase offset ;
+-----------------+--------------------+----------+------------------+---------------+--------------+----------+-----------------------+---------------------+--------+--------------+
; clock           ;                    ; User Pin ; None             ; 0.000 ns      ; 0.000 ns     ; --       ; N/A                   ; N/A                 ; N/A    ;              ;
+-----------------+--------------------+----------+------------------+---------------+--------------+----------+-----------------------+---------------------+--------+--------------+


Parallel compilation was disabled, but you have multiple processors available. Enable parallel compilation to reduce compilation time.
+-------------------------------------+
; Parallel Compilation                ;
+----------------------------+--------+
; Processors                 ; Number ;
+----------------------------+--------+
; Number detected on machine ; 2      ;
; Maximum allowed            ; 1      ;
+----------------------------+--------+


+--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; Clock Setup: 'clock'                                                                                                                                                                                                                                               ;
+-----------------------------------------+-----------------------------------------------------+---------------------------+----------------------------+------------+----------+-----------------------------+---------------------------+-------------------------+
; Slack                                   ; Actual fmax (period)                                ; From                      ; To                         ; From Clock ; To Clock ; Required Setup Relationship ; Required Longest P2P Time ; Actual Longest P2P Time ;
+-----------------------------------------+-----------------------------------------------------+---------------------------+----------------------------+------------+----------+-----------------------------+---------------------------+-------------------------+
; N/A                                     ; 86.93 MHz ( period = 11.504 ns )                    ; freq_div:inst|counter[7]  ; freq_div:inst|counter[100] ; clock      ; clock    ; None                        ; None                      ; 11.275 ns               ;
; N/A                                     ; 87.43 MHz ( period = 11.438 ns )                    ; freq_div:inst|counter[7]  ; freq_div:inst|counter[95]  ; clock      ; clock    ; None                        ; None                      ; 11.210 ns               ;
; N/A                                     ; 87.61 MHz ( period = 11.414 ns )                    ; freq_div:inst|counter[9]  ; freq_div:inst|counter[100] ; clock      ; clock    ; None                        ; None                      ; 11.185 ns               ;
; N/A                                     ; 88.04 MHz ( period = 11.359 ns )                    ; freq_div:inst|counter[0]  ; freq_div:inst|counter[100] ; clock      ; clock    ; None                        ; None                      ; 11.145 ns               ;
; N/A                                     ; 88.11 MHz ( period = 11.349 ns )                    ; freq_div:inst|counter[7]  ; freq_div:inst|counter[94]  ; clock      ; clock    ; None                        ; None                      ; 11.121 ns               ;
; N/A                                     ; 88.12 MHz ( period = 11.348 ns )                    ; freq_div:inst|counter[9]  ; freq_div:inst|counter[95]  ; clock      ; clock    ; None                        ; None                      ; 11.120 ns               ;
; N/A                                     ; 88.16 MHz ( period = 11.343 ns )                    ; freq_div:inst|counter[7]  ; freq_div:inst|counter[98]  ; clock      ; clock    ; None                        ; None                      ; 11.114 ns               ;
; N/A                                     ; 88.55 MHz ( period = 11.293 ns )                    ; freq_div:inst|counter[0]  ; freq_div:inst|counter[95]  ; clock      ; clock    ; None                        ; None                      ; 11.080 ns               ;
; N/A                                     ; 88.64 MHz ( period = 11.281 ns )                    ; freq_div:inst|counter[7]  ; freq_div:inst|counter[93]  ; clock      ; clock    ; None                        ; None                      ; 11.053 ns               ;
; N/A                                     ; 88.74 MHz ( period = 11.269 ns )                    ; freq_div:inst|counter[7]  ; freq_div:inst|counter[99]  ; clock      ; clock    ; None                        ; None                      ; 11.040 ns               ;
; N/A                                     ; 88.82 MHz ( period = 11.259 ns )                    ; freq_div:inst|counter[9]  ; freq_div:inst|counter[94]  ; clock      ; clock    ; None                        ; None                      ; 11.031 ns               ;
; N/A                                     ; 88.87 MHz ( period = 11.253 ns )                    ; freq_div:inst|counter[9]  ; freq_div:inst|counter[98]  ; clock      ; clock    ; None                        ; None                      ; 11.024 ns               ;
; N/A                                     ; 88.93 MHz ( period = 11.245 ns )                    ; freq_div:inst|counter[1]  ; freq_div:inst|counter[100] ; clock      ; clock    ; None                        ; None                      ; 11.031 ns               ;
; N/A                                     ; 89.25 MHz ( period = 11.204 ns )                    ; freq_div:inst|counter[0]  ; freq_div:inst|counter[94]  ; clock      ; clock    ; None                        ; None                      ; 10.991 ns               ;
; N/A                                     ; 89.30 MHz ( period = 11.198 ns )                    ; freq_div:inst|counter[0]  ; freq_div:inst|counter[98]  ; clock      ; clock    ; None                        ; None                      ; 10.984 ns               ;
; N/A                                     ; 89.36 MHz ( period = 11.191 ns )                    ; freq_div:inst|counter[9]  ; freq_div:inst|counter[93]  ; clock      ; clock    ; None                        ; None                      ; 10.963 ns               ;
; N/A                                     ; 89.40 MHz ( period = 11.186 ns )                    ; freq_div:inst|counter[7]  ; freq_div:inst|counter[89]  ; clock      ; clock    ; None                        ; None                      ; 10.951 ns               ;
; N/A                                     ; 89.45 MHz ( period = 11.179 ns )                    ; freq_div:inst|counter[1]  ; freq_div:inst|counter[95]  ; clock      ; clock    ; None                        ; None                      ; 10.966 ns               ;
; N/A                                     ; 89.45 MHz ( period = 11.179 ns )                    ; freq_div:inst|counter[9]  ; freq_div:inst|counter[99]  ; clock      ; clock    ; None                        ; None                      ; 10.950 ns               ;
; N/A                                     ; 89.57 MHz ( period = 11.164 ns )                    ; freq_div:inst|counter[7]  ; freq_div:inst|counter[92]  ; clock      ; clock    ; None                        ; None                      ; 10.929 ns               ;
; N/A                                     ; 89.60 MHz ( period = 11.161 ns )                    ; freq_div:inst|counter[7]  ; freq_div:inst|counter[97]  ; clock      ; clock    ; None                        ; None                      ; 10.932 ns               ;
; N/A                                     ; 89.80 MHz ( period = 11.136 ns )                    ; freq_div:inst|counter[0]  ; freq_div:inst|counter[93]  ; clock      ; clock    ; None                        ; None                      ; 10.923 ns               ;
; N/A                                     ; 89.90 MHz ( period = 11.124 ns )                    ; freq_div:inst|counter[0]  ; freq_div:inst|counter[99]  ; clock      ; clock    ; None                        ; None                      ; 10.910 ns               ;
; N/A                                     ; 90.03 MHz ( period = 11.108 ns )                    ; freq_div:inst|counter[2]  ; freq_div:inst|counter[100] ; clock      ; clock    ; None                        ; None                      ; 10.894 ns               ;
; N/A                                     ; 90.12 MHz ( period = 11.096 ns )                    ; freq_div:inst|counter[9]  ; freq_div:inst|counter[89]  ; clock      ; clock    ; None                        ; None                      ; 10.861 ns               ;
; N/A                                     ; 90.17 MHz ( period = 11.090 ns )                    ; freq_div:inst|counter[1]  ; freq_div:inst|counter[94]  ; clock      ; clock    ; None                        ; None                      ; 10.877 ns               ;
; N/A                                     ; 90.18 MHz ( period = 11.089 ns )                    ; freq_div:inst|counter[7]  ; freq_div:inst|counter[91]  ; clock      ; clock    ; None                        ; None                      ; 10.854 ns               ;
; N/A                                     ; 90.22 MHz ( period = 11.084 ns )                    ; freq_div:inst|counter[1]  ; freq_div:inst|counter[98]  ; clock      ; clock    ; None                        ; None                      ; 10.870 ns               ;
; N/A                                     ; 90.30 MHz ( period = 11.074 ns )                    ; freq_div:inst|counter[9]  ; freq_div:inst|counter[92]  ; clock      ; clock    ; None                        ; None                      ; 10.839 ns               ;
; N/A                                     ; 90.33 MHz ( period = 11.071 ns )                    ; freq_div:inst|counter[9]  ; freq_div:inst|counter[97]  ; clock      ; clock    ; None                        ; None                      ; 10.842 ns               ;
; N/A                                     ; 90.56 MHz ( period = 11.042 ns )                    ; freq_div:inst|counter[2]  ; freq_div:inst|counter[95]  ; clock      ; clock    ; None                        ; None                      ; 10.829 ns               ;
; N/A                                     ; 90.57 MHz ( period = 11.041 ns )                    ; freq_div:inst|counter[0]  ; freq_div:inst|counter[89]  ; clock      ; clock    ; None                        ; None                      ; 10.821 ns               ;
; N/A                                     ; 90.73 MHz ( period = 11.022 ns )                    ; freq_div:inst|counter[1]  ; freq_div:inst|counter[93]  ; clock      ; clock    ; None                        ; None                      ; 10.809 ns               ;
; N/A                                     ; 90.75 MHz ( period = 11.019 ns )                    ; freq_div:inst|counter[0]  ; freq_div:inst|counter[92]  ; clock      ; clock    ; None                        ; None                      ; 10.799 ns               ;
; N/A                                     ; 90.78 MHz ( period = 11.016 ns )                    ; freq_div:inst|counter[0]  ; freq_div:inst|counter[97]  ; clock      ; clock    ; None                        ; None                      ; 10.802 ns               ;
; N/A                                     ; 90.82 MHz ( period = 11.011 ns )                    ; freq_div:inst|counter[7]  ; freq_div:inst|counter[90]  ; clock      ; clock    ; None                        ; None                      ; 10.776 ns               ;
; N/A                                     ; 90.83 MHz ( period = 11.010 ns )                    ; freq_div:inst|counter[1]  ; freq_div:inst|counter[99]  ; clock      ; clock    ; None                        ; None                      ; 10.796 ns               ;
; N/A                                     ; 90.92 MHz ( period = 10.999 ns )                    ; freq_div:inst|counter[9]  ; freq_div:inst|counter[91]  ; clock      ; clock    ; None                        ; None                      ; 10.764 ns               ;
; N/A                                     ; 91.02 MHz ( period = 10.987 ns )                    ; freq_div:inst|counter[3]  ; freq_div:inst|counter[100] ; clock      ; clock    ; None                        ; None                      ; 10.773 ns               ;
; N/A                                     ; 91.09 MHz ( period = 10.978 ns )                    ; freq_div:inst|counter[13] ; freq_div:inst|counter[100] ; clock      ; clock    ; None                        ; None                      ; 10.749 ns               ;
; N/A                                     ; 91.30 MHz ( period = 10.953 ns )                    ; freq_div:inst|counter[2]  ; freq_div:inst|counter[94]  ; clock      ; clock    ; None                        ; None                      ; 10.740 ns               ;
; N/A                                     ; 91.35 MHz ( period = 10.947 ns )                    ; freq_div:inst|counter[2]  ; freq_div:inst|counter[98]  ; clock      ; clock    ; None                        ; None                      ; 10.733 ns               ;
; N/A                                     ; 91.37 MHz ( period = 10.944 ns )                    ; freq_div:inst|counter[0]  ; freq_div:inst|counter[91]  ; clock      ; clock    ; None                        ; None                      ; 10.724 ns               ;
; N/A                                     ; 91.47 MHz ( period = 10.932 ns )                    ; freq_div:inst|counter[7]  ; freq_div:inst|counter[96]  ; clock      ; clock    ; None                        ; None                      ; 10.703 ns               ;
; N/A                                     ; 91.52 MHz ( period = 10.927 ns )                    ; freq_div:inst|counter[1]  ; freq_div:inst|counter[89]  ; clock      ; clock    ; None                        ; None                      ; 10.707 ns               ;
; N/A                                     ; 91.57 MHz ( period = 10.921 ns )                    ; freq_div:inst|counter[9]  ; freq_div:inst|counter[90]  ; clock      ; clock    ; None                        ; None                      ; 10.686 ns               ;
; N/A                                     ; 91.57 MHz ( period = 10.921 ns )                    ; freq_div:inst|counter[3]  ; freq_div:inst|counter[95]  ; clock      ; clock    ; None                        ; None                      ; 10.708 ns               ;
; N/A                                     ; 91.64 MHz ( period = 10.912 ns )                    ; freq_div:inst|counter[13] ; freq_div:inst|counter[95]  ; clock      ; clock    ; None                        ; None                      ; 10.684 ns               ;
; N/A                                     ; 91.68 MHz ( period = 10.908 ns )                    ; freq_div:inst|counter[4]  ; freq_div:inst|counter[100] ; clock      ; clock    ; None                        ; None                      ; 10.694 ns               ;
; N/A                                     ; 91.70 MHz ( period = 10.905 ns )                    ; freq_div:inst|counter[1]  ; freq_div:inst|counter[92]  ; clock      ; clock    ; None                        ; None                      ; 10.685 ns               ;
; N/A                                     ; 91.73 MHz ( period = 10.902 ns )                    ; freq_div:inst|counter[1]  ; freq_div:inst|counter[97]  ; clock      ; clock    ; None                        ; None                      ; 10.688 ns               ;
; N/A                                     ; 91.87 MHz ( period = 10.885 ns )                    ; freq_div:inst|counter[2]  ; freq_div:inst|counter[93]  ; clock      ; clock    ; None                        ; None                      ; 10.672 ns               ;
; N/A                                     ; 91.97 MHz ( period = 10.873 ns )                    ; freq_div:inst|counter[2]  ; freq_div:inst|counter[99]  ; clock      ; clock    ; None                        ; None                      ; 10.659 ns               ;
; N/A                                     ; 92.03 MHz ( period = 10.866 ns )                    ; freq_div:inst|counter[0]  ; freq_div:inst|counter[90]  ; clock      ; clock    ; None                        ; None                      ; 10.646 ns               ;
; N/A                                     ; 92.23 MHz ( period = 10.842 ns )                    ; freq_div:inst|counter[4]  ; freq_div:inst|counter[95]  ; clock      ; clock    ; None                        ; None                      ; 10.629 ns               ;
; N/A                                     ; 92.23 MHz ( period = 10.842 ns )                    ; freq_div:inst|counter[9]  ; freq_div:inst|counter[96]  ; clock      ; clock    ; None                        ; None                      ; 10.613 ns               ;
; N/A                                     ; 92.32 MHz ( period = 10.832 ns )                    ; freq_div:inst|counter[3]  ; freq_div:inst|counter[94]  ; clock      ; clock    ; None                        ; None                      ; 10.619 ns               ;
; N/A                                     ; 92.34 MHz ( period = 10.830 ns )                    ; freq_div:inst|counter[1]  ; freq_div:inst|counter[91]  ; clock      ; clock    ; None                        ; None                      ; 10.610 ns               ;
; N/A                                     ; 92.37 MHz ( period = 10.826 ns )                    ; freq_div:inst|counter[3]  ; freq_div:inst|counter[98]  ; clock      ; clock    ; None                        ; None                      ; 10.612 ns               ;
; N/A                                     ; 92.40 MHz ( period = 10.823 ns )                    ; freq_div:inst|counter[13] ; freq_div:inst|counter[94]  ; clock      ; clock    ; None                        ; None                      ; 10.595 ns               ;
; N/A                                     ; 92.44 MHz ( period = 10.818 ns )                    ; freq_div:inst|counter[5]  ; freq_div:inst|counter[100] ; clock      ; clock    ; None                        ; None                      ; 10.604 ns               ;
; N/A                                     ; 92.45 MHz ( period = 10.817 ns )                    ; freq_div:inst|counter[13] ; freq_div:inst|counter[98]  ; clock      ; clock    ; None                        ; None                      ; 10.588 ns               ;
; N/A                                     ; 92.68 MHz ( period = 10.790 ns )                    ; freq_div:inst|counter[2]  ; freq_div:inst|counter[89]  ; clock      ; clock    ; None                        ; None                      ; 10.570 ns               ;
; N/A                                     ; 92.70 MHz ( period = 10.787 ns )                    ; freq_div:inst|counter[0]  ; freq_div:inst|counter[96]  ; clock      ; clock    ; None                        ; None                      ; 10.573 ns               ;
; N/A                                     ; 92.73 MHz ( period = 10.784 ns )                    ; freq_div:inst|counter[7]  ; freq_div:inst|counter[84]  ; clock      ; clock    ; None                        ; None                      ; 10.549 ns               ;
; N/A                                     ; 92.74 MHz ( period = 10.783 ns )                    ; freq_div:inst|counter[6]  ; freq_div:inst|counter[100] ; clock      ; clock    ; None                        ; None                      ; 10.569 ns               ;
; N/A                                     ; 92.87 MHz ( period = 10.768 ns )                    ; freq_div:inst|counter[2]  ; freq_div:inst|counter[92]  ; clock      ; clock    ; None                        ; None                      ; 10.548 ns               ;
; N/A                                     ; 92.89 MHz ( period = 10.765 ns )                    ; freq_div:inst|counter[2]  ; freq_div:inst|counter[97]  ; clock      ; clock    ; None                        ; None                      ; 10.551 ns               ;
; N/A                                     ; 92.90 MHz ( period = 10.764 ns )                    ; freq_div:inst|counter[3]  ; freq_div:inst|counter[93]  ; clock      ; clock    ; None                        ; None                      ; 10.551 ns               ;
; N/A                                     ; 92.91 MHz ( period = 10.763 ns )                    ; freq_div:inst|counter[7]  ; freq_div:inst|counter[88]  ; clock      ; clock    ; None                        ; None                      ; 10.535 ns               ;
; N/A                                     ; 92.95 MHz ( period = 10.759 ns )                    ; freq_div:inst|counter[7]  ; freq_div:inst|counter[86]  ; clock      ; clock    ; None                        ; None                      ; 10.531 ns               ;
; N/A                                     ; 92.98 MHz ( period = 10.755 ns )                    ; freq_div:inst|counter[13] ; freq_div:inst|counter[93]  ; clock      ; clock    ; None                        ; None                      ; 10.527 ns               ;
; N/A                                     ; 93.00 MHz ( period = 10.753 ns )                    ; freq_div:inst|counter[4]  ; freq_div:inst|counter[94]  ; clock      ; clock    ; None                        ; None                      ; 10.540 ns               ;
; N/A                                     ; 93.01 MHz ( period = 10.752 ns )                    ; freq_div:inst|counter[1]  ; freq_div:inst|counter[90]  ; clock      ; clock    ; None                        ; None                      ; 10.532 ns               ;
; N/A                                     ; 93.01 MHz ( period = 10.752 ns )                    ; freq_div:inst|counter[5]  ; freq_div:inst|counter[95]  ; clock      ; clock    ; None                        ; None                      ; 10.539 ns               ;
; N/A                                     ; 93.01 MHz ( period = 10.752 ns )                    ; freq_div:inst|counter[3]  ; freq_div:inst|counter[99]  ; clock      ; clock    ; None                        ; None                      ; 10.538 ns               ;
; N/A                                     ; 93.05 MHz ( period = 10.747 ns )                    ; freq_div:inst|counter[4]  ; freq_div:inst|counter[98]  ; clock      ; clock    ; None                        ; None                      ; 10.533 ns               ;
; N/A                                     ; 93.08 MHz ( period = 10.743 ns )                    ; freq_div:inst|counter[13] ; freq_div:inst|counter[99]  ; clock      ; clock    ; None                        ; None                      ; 10.514 ns               ;
; N/A                                     ; 93.21 MHz ( period = 10.729 ns )                    ; freq_div:inst|counter[7]  ; freq_div:inst|counter[87]  ; clock      ; clock    ; None                        ; None                      ; 10.501 ns               ;
; N/A                                     ; 93.31 MHz ( period = 10.717 ns )                    ; freq_div:inst|counter[6]  ; freq_div:inst|counter[95]  ; clock      ; clock    ; None                        ; None                      ; 10.504 ns               ;
; N/A                                     ; 93.35 MHz ( period = 10.712 ns )                    ; freq_div:inst|counter[7]  ; freq_div:inst|counter[85]  ; clock      ; clock    ; None                        ; None                      ; 10.484 ns               ;
; N/A                                     ; 93.48 MHz ( period = 10.698 ns )                    ; freq_div:inst|counter[7]  ; freq_div:inst|counter[83]  ; clock      ; clock    ; None                        ; None                      ; 10.463 ns               ;
; N/A                                     ; 93.51 MHz ( period = 10.694 ns )                    ; freq_div:inst|counter[9]  ; freq_div:inst|counter[84]  ; clock      ; clock    ; None                        ; None                      ; 10.459 ns               ;
; N/A                                     ; 93.52 MHz ( period = 10.693 ns )                    ; freq_div:inst|counter[2]  ; freq_div:inst|counter[91]  ; clock      ; clock    ; None                        ; None                      ; 10.473 ns               ;
; N/A                                     ; 93.59 MHz ( period = 10.685 ns )                    ; freq_div:inst|counter[4]  ; freq_div:inst|counter[93]  ; clock      ; clock    ; None                        ; None                      ; 10.472 ns               ;
; N/A                                     ; 93.69 MHz ( period = 10.673 ns )                    ; freq_div:inst|counter[9]  ; freq_div:inst|counter[88]  ; clock      ; clock    ; None                        ; None                      ; 10.445 ns               ;
; N/A                                     ; 93.69 MHz ( period = 10.673 ns )                    ; freq_div:inst|counter[1]  ; freq_div:inst|counter[96]  ; clock      ; clock    ; None                        ; None                      ; 10.459 ns               ;
; N/A                                     ; 93.69 MHz ( period = 10.673 ns )                    ; freq_div:inst|counter[4]  ; freq_div:inst|counter[99]  ; clock      ; clock    ; None                        ; None                      ; 10.459 ns               ;
; N/A                                     ; 93.73 MHz ( period = 10.669 ns )                    ; freq_div:inst|counter[9]  ; freq_div:inst|counter[86]  ; clock      ; clock    ; None                        ; None                      ; 10.441 ns               ;
; N/A                                     ; 93.73 MHz ( period = 10.669 ns )                    ; freq_div:inst|counter[3]  ; freq_div:inst|counter[89]  ; clock      ; clock    ; None                        ; None                      ; 10.449 ns               ;
; N/A                                     ; 93.78 MHz ( period = 10.663 ns )                    ; freq_div:inst|counter[5]  ; freq_div:inst|counter[94]  ; clock      ; clock    ; None                        ; None                      ; 10.450 ns               ;
; N/A                                     ; 93.81 MHz ( period = 10.660 ns )                    ; freq_div:inst|counter[13] ; freq_div:inst|counter[89]  ; clock      ; clock    ; None                        ; None                      ; 10.425 ns               ;
; N/A                                     ; 93.84 MHz ( period = 10.657 ns )                    ; freq_div:inst|counter[5]  ; freq_div:inst|counter[98]  ; clock      ; clock    ; None                        ; None                      ; 10.443 ns               ;
; N/A                                     ; 93.92 MHz ( period = 10.647 ns )                    ; freq_div:inst|counter[3]  ; freq_div:inst|counter[92]  ; clock      ; clock    ; None                        ; None                      ; 10.427 ns               ;
; N/A                                     ; 93.95 MHz ( period = 10.644 ns )                    ; freq_div:inst|counter[3]  ; freq_div:inst|counter[97]  ; clock      ; clock    ; None                        ; None                      ; 10.430 ns               ;
; N/A                                     ; 93.99 MHz ( period = 10.639 ns )                    ; freq_div:inst|counter[9]  ; freq_div:inst|counter[87]  ; clock      ; clock    ; None                        ; None                      ; 10.411 ns               ;
; N/A                                     ; 93.99 MHz ( period = 10.639 ns )                    ; freq_div:inst|counter[0]  ; freq_div:inst|counter[84]  ; clock      ; clock    ; None                        ; None                      ; 10.419 ns               ;
; N/A                                     ; 94.00 MHz ( period = 10.638 ns )                    ; freq_div:inst|counter[13] ; freq_div:inst|counter[92]  ; clock      ; clock    ; None                        ; None                      ; 10.403 ns               ;
; N/A                                     ; 94.03 MHz ( period = 10.635 ns )                    ; freq_div:inst|counter[13] ; freq_div:inst|counter[97]  ; clock      ; clock    ; None                        ; None                      ; 10.406 ns               ;
; N/A                                     ; 94.09 MHz ( period = 10.628 ns )                    ; freq_div:inst|counter[6]  ; freq_div:inst|counter[94]  ; clock      ; clock    ; None                        ; None                      ; 10.415 ns               ;
; N/A                                     ; 94.14 MHz ( period = 10.622 ns )                    ; freq_div:inst|counter[9]  ; freq_div:inst|counter[85]  ; clock      ; clock    ; None                        ; None                      ; 10.394 ns               ;
; N/A                                     ; 94.14 MHz ( period = 10.622 ns )                    ; freq_div:inst|counter[6]  ; freq_div:inst|counter[98]  ; clock      ; clock    ; None                        ; None                      ; 10.408 ns               ;
; N/A                                     ; 94.18 MHz ( period = 10.618 ns )                    ; freq_div:inst|counter[0]  ; freq_div:inst|counter[88]  ; clock      ; clock    ; None                        ; None                      ; 10.405 ns               ;
; N/A                                     ; 94.21 MHz ( period = 10.615 ns )                    ; freq_div:inst|counter[2]  ; freq_div:inst|counter[90]  ; clock      ; clock    ; None                        ; None                      ; 10.395 ns               ;
; N/A                                     ; 94.22 MHz ( period = 10.614 ns )                    ; freq_div:inst|counter[0]  ; freq_div:inst|counter[86]  ; clock      ; clock    ; None                        ; None                      ; 10.401 ns               ;
; N/A                                     ; 94.27 MHz ( period = 10.608 ns )                    ; freq_div:inst|counter[9]  ; freq_div:inst|counter[83]  ; clock      ; clock    ; None                        ; None                      ; 10.373 ns               ;
; N/A                                     ; 94.38 MHz ( period = 10.595 ns )                    ; freq_div:inst|counter[5]  ; freq_div:inst|counter[93]  ; clock      ; clock    ; None                        ; None                      ; 10.382 ns               ;
; N/A                                     ; 94.43 MHz ( period = 10.590 ns )                    ; freq_div:inst|counter[4]  ; freq_div:inst|counter[89]  ; clock      ; clock    ; None                        ; None                      ; 10.370 ns               ;
; N/A                                     ; 94.48 MHz ( period = 10.584 ns )                    ; freq_div:inst|counter[0]  ; freq_div:inst|counter[87]  ; clock      ; clock    ; None                        ; None                      ; 10.371 ns               ;
; N/A                                     ; 94.49 MHz ( period = 10.583 ns )                    ; freq_div:inst|counter[5]  ; freq_div:inst|counter[99]  ; clock      ; clock    ; None                        ; None                      ; 10.369 ns               ;
; N/A                                     ; 94.56 MHz ( period = 10.575 ns )                    ; freq_div:inst|counter[8]  ; freq_div:inst|counter[100] ; clock      ; clock    ; None                        ; None                      ; 10.361 ns               ;
; N/A                                     ; 94.59 MHz ( period = 10.572 ns )                    ; freq_div:inst|counter[3]  ; freq_div:inst|counter[91]  ; clock      ; clock    ; None                        ; None                      ; 10.352 ns               ;
; N/A                                     ; 94.63 MHz ( period = 10.568 ns )                    ; freq_div:inst|counter[4]  ; freq_div:inst|counter[92]  ; clock      ; clock    ; None                        ; None                      ; 10.348 ns               ;
; N/A                                     ; 94.63 MHz ( period = 10.567 ns )                    ; freq_div:inst|counter[0]  ; freq_div:inst|counter[85]  ; clock      ; clock    ; None                        ; None                      ; 10.354 ns               ;
; N/A                                     ; 94.65 MHz ( period = 10.565 ns )                    ; freq_div:inst|counter[4]  ; freq_div:inst|counter[97]  ; clock      ; clock    ; None                        ; None                      ; 10.351 ns               ;
; N/A                                     ; 94.67 MHz ( period = 10.563 ns )                    ; freq_div:inst|counter[13] ; freq_div:inst|counter[91]  ; clock      ; clock    ; None                        ; None                      ; 10.328 ns               ;
; N/A                                     ; 94.70 MHz ( period = 10.560 ns )                    ; freq_div:inst|counter[6]  ; freq_div:inst|counter[93]  ; clock      ; clock    ; None                        ; None                      ; 10.347 ns               ;
; N/A                                     ; 94.76 MHz ( period = 10.553 ns )                    ; freq_div:inst|counter[0]  ; freq_div:inst|counter[83]  ; clock      ; clock    ; None                        ; None                      ; 10.333 ns               ;
; N/A                                     ; 94.80 MHz ( period = 10.548 ns )                    ; freq_div:inst|counter[6]  ; freq_div:inst|counter[99]  ; clock      ; clock    ; None                        ; None                      ; 10.334 ns               ;
; N/A                                     ; 94.91 MHz ( period = 10.536 ns )                    ; freq_div:inst|counter[2]  ; freq_div:inst|counter[96]  ; clock      ; clock    ; None                        ; None                      ; 10.322 ns               ;
; N/A                                     ; 95.01 MHz ( period = 10.525 ns )                    ; freq_div:inst|counter[1]  ; freq_div:inst|counter[84]  ; clock      ; clock    ; None                        ; None                      ; 10.305 ns               ;
; N/A                                     ; 95.16 MHz ( period = 10.509 ns )                    ; freq_div:inst|counter[8]  ; freq_div:inst|counter[95]  ; clock      ; clock    ; None                        ; None                      ; 10.296 ns               ;
; N/A                                     ; 95.20 MHz ( period = 10.504 ns )                    ; freq_div:inst|counter[1]  ; freq_div:inst|counter[88]  ; clock      ; clock    ; None                        ; None                      ; 10.291 ns               ;
; N/A                                     ; 95.24 MHz ( period = 10.500 ns )                    ; freq_div:inst|counter[1]  ; freq_div:inst|counter[86]  ; clock      ; clock    ; None                        ; None                      ; 10.287 ns               ;
; N/A                                     ; 95.24 MHz ( period = 10.500 ns )                    ; freq_div:inst|counter[5]  ; freq_div:inst|counter[89]  ; clock      ; clock    ; None                        ; None                      ; 10.280 ns               ;
; N/A                                     ; 95.29 MHz ( period = 10.494 ns )                    ; freq_div:inst|counter[3]  ; freq_div:inst|counter[90]  ; clock      ; clock    ; None                        ; None                      ; 10.274 ns               ;
; N/A                                     ; 95.30 MHz ( period = 10.493 ns )                    ; freq_div:inst|counter[4]  ; freq_div:inst|counter[91]  ; clock      ; clock    ; None                        ; None                      ; 10.273 ns               ;
; N/A                                     ; 95.37 MHz ( period = 10.485 ns )                    ; freq_div:inst|counter[13] ; freq_div:inst|counter[90]  ; clock      ; clock    ; None                        ; None                      ; 10.250 ns               ;
; N/A                                     ; 95.37 MHz ( period = 10.485 ns )                    ; freq_div:inst|counter[16] ; freq_div:inst|counter[100] ; clock      ; clock    ; None                        ; None                      ; 10.254 ns               ;
; N/A                                     ; 95.43 MHz ( period = 10.479 ns )                    ; freq_div:inst|counter[7]  ; freq_div:inst|counter[81]  ; clock      ; clock    ; None                        ; None                      ; 10.244 ns               ;
; N/A                                     ; 95.44 MHz ( period = 10.478 ns )                    ; freq_div:inst|counter[5]  ; freq_div:inst|counter[92]  ; clock      ; clock    ; None                        ; None                      ; 10.258 ns               ;
; N/A                                     ; 95.47 MHz ( period = 10.475 ns )                    ; freq_div:inst|counter[5]  ; freq_div:inst|counter[97]  ; clock      ; clock    ; None                        ; None                      ; 10.261 ns               ;
; N/A                                     ; 95.51 MHz ( period = 10.470 ns )                    ; freq_div:inst|counter[1]  ; freq_div:inst|counter[87]  ; clock      ; clock    ; None                        ; None                      ; 10.257 ns               ;
; N/A                                     ; 95.56 MHz ( period = 10.465 ns )                    ; freq_div:inst|counter[6]  ; freq_div:inst|counter[89]  ; clock      ; clock    ; None                        ; None                      ; 10.245 ns               ;
; N/A                                     ; 95.57 MHz ( period = 10.464 ns )                    ; freq_div:inst|counter[15] ; freq_div:inst|counter[100] ; clock      ; clock    ; None                        ; None                      ; 10.235 ns               ;
; N/A                                     ; 95.67 MHz ( period = 10.453 ns )                    ; freq_div:inst|counter[1]  ; freq_div:inst|counter[85]  ; clock      ; clock    ; None                        ; None                      ; 10.240 ns               ;
; N/A                                     ; 95.68 MHz ( period = 10.451 ns )                    ; freq_div:inst|counter[7]  ; freq_div:inst|counter[80]  ; clock      ; clock    ; None                        ; None                      ; 10.216 ns               ;
; N/A                                     ; 95.76 MHz ( period = 10.443 ns )                    ; freq_div:inst|counter[6]  ; freq_div:inst|counter[92]  ; clock      ; clock    ; None                        ; None                      ; 10.223 ns               ;
; N/A                                     ; 95.79 MHz ( period = 10.440 ns )                    ; freq_div:inst|counter[6]  ; freq_div:inst|counter[97]  ; clock      ; clock    ; None                        ; None                      ; 10.226 ns               ;
; N/A                                     ; 95.79 MHz ( period = 10.439 ns )                    ; freq_div:inst|counter[1]  ; freq_div:inst|counter[83]  ; clock      ; clock    ; None                        ; None                      ; 10.219 ns               ;
; N/A                                     ; 95.93 MHz ( period = 10.424 ns )                    ; freq_div:inst|counter[7]  ; freq_div:inst|counter[82]  ; clock      ; clock    ; None                        ; None                      ; 10.189 ns               ;
; N/A                                     ; 95.97 MHz ( period = 10.420 ns )                    ; freq_div:inst|counter[8]  ; freq_div:inst|counter[94]  ; clock      ; clock    ; None                        ; None                      ; 10.207 ns               ;
; N/A                                     ; 95.98 MHz ( period = 10.419 ns )                    ; freq_div:inst|counter[16] ; freq_div:inst|counter[95]  ; clock      ; clock    ; None                        ; None                      ; 10.189 ns               ;
; N/A                                     ; 95.98 MHz ( period = 10.419 ns )                    ; freq_div:inst|counter[7]  ; freq_div:inst|counter[79]  ; clock      ; clock    ; None                        ; None                      ; 10.184 ns               ;
; N/A                                     ; 96.02 MHz ( period = 10.415 ns )                    ; freq_div:inst|counter[4]  ; freq_div:inst|counter[90]  ; clock      ; clock    ; None                        ; None                      ; 10.195 ns               ;
; N/A                                     ; 96.02 MHz ( period = 10.415 ns )                    ; freq_div:inst|counter[3]  ; freq_div:inst|counter[96]  ; clock      ; clock    ; None                        ; None                      ; 10.201 ns               ;
; N/A                                     ; 96.02 MHz ( period = 10.414 ns )                    ; freq_div:inst|counter[8]  ; freq_div:inst|counter[98]  ; clock      ; clock    ; None                        ; None                      ; 10.200 ns               ;
; N/A                                     ; 96.04 MHz ( period = 10.412 ns )                    ; freq_div:inst|counter[19] ; freq_div:inst|counter[100] ; clock      ; clock    ; None                        ; None                      ; 10.183 ns               ;
; N/A                                     ; 96.10 MHz ( period = 10.406 ns )                    ; freq_div:inst|counter[13] ; freq_div:inst|counter[96]  ; clock      ; clock    ; None                        ; None                      ; 10.177 ns               ;
; N/A                                     ; 96.13 MHz ( period = 10.403 ns )                    ; freq_div:inst|counter[5]  ; freq_div:inst|counter[91]  ; clock      ; clock    ; None                        ; None                      ; 10.183 ns               ;
; N/A                                     ; 96.17 MHz ( period = 10.398 ns )                    ; freq_div:inst|counter[15] ; freq_div:inst|counter[95]  ; clock      ; clock    ; None                        ; None                      ; 10.170 ns               ;
; N/A                                     ; 96.26 MHz ( period = 10.389 ns )                    ; freq_div:inst|counter[9]  ; freq_div:inst|counter[81]  ; clock      ; clock    ; None                        ; None                      ; 10.154 ns               ;
; N/A                                     ; 96.26 MHz ( period = 10.388 ns )                    ; freq_div:inst|counter[2]  ; freq_div:inst|counter[84]  ; clock      ; clock    ; None                        ; None                      ; 10.168 ns               ;
; N/A                                     ; 96.45 MHz ( period = 10.368 ns )                    ; freq_div:inst|counter[6]  ; freq_div:inst|counter[91]  ; clock      ; clock    ; None                        ; None                      ; 10.148 ns               ;
; N/A                                     ; 96.46 MHz ( period = 10.367 ns )                    ; freq_div:inst|counter[2]  ; freq_div:inst|counter[88]  ; clock      ; clock    ; None                        ; None                      ; 10.154 ns               ;
; N/A                                     ; 96.50 MHz ( period = 10.363 ns )                    ; freq_div:inst|counter[2]  ; freq_div:inst|counter[86]  ; clock      ; clock    ; None                        ; None                      ; 10.150 ns               ;
; N/A                                     ; 96.52 MHz ( period = 10.361 ns )                    ; freq_div:inst|counter[9]  ; freq_div:inst|counter[80]  ; clock      ; clock    ; None                        ; None                      ; 10.126 ns               ;
; N/A                                     ; 96.60 MHz ( period = 10.352 ns )                    ; freq_div:inst|counter[8]  ; freq_div:inst|counter[93]  ; clock      ; clock    ; None                        ; None                      ; 10.139 ns               ;
; N/A                                     ; 96.66 MHz ( period = 10.346 ns )                    ; freq_div:inst|counter[19] ; freq_div:inst|counter[95]  ; clock      ; clock    ; None                        ; None                      ; 10.118 ns               ;
; N/A                                     ; 96.69 MHz ( period = 10.342 ns )                    ; freq_div:inst|counter[10] ; freq_div:inst|counter[100] ; clock      ; clock    ; None                        ; None                      ; 10.120 ns               ;
; N/A                                     ; 96.71 MHz ( period = 10.340 ns )                    ; freq_div:inst|counter[8]  ; freq_div:inst|counter[99]  ; clock      ; clock    ; None                        ; None                      ; 10.126 ns               ;
; N/A                                     ; 96.75 MHz ( period = 10.336 ns )                    ; freq_div:inst|counter[4]  ; freq_div:inst|counter[96]  ; clock      ; clock    ; None                        ; None                      ; 10.122 ns               ;
; N/A                                     ; 96.77 MHz ( period = 10.334 ns )                    ; freq_div:inst|counter[9]  ; freq_div:inst|counter[82]  ; clock      ; clock    ; None                        ; None                      ; 10.099 ns               ;
; N/A                                     ; 96.77 MHz ( period = 10.334 ns )                    ; freq_div:inst|counter[0]  ; freq_div:inst|counter[81]  ; clock      ; clock    ; None                        ; None                      ; 10.114 ns               ;
; N/A                                     ; 96.78 MHz ( period = 10.333 ns )                    ; freq_div:inst|counter[2]  ; freq_div:inst|counter[87]  ; clock      ; clock    ; None                        ; None                      ; 10.120 ns               ;
; N/A                                     ; 96.81 MHz ( period = 10.330 ns )                    ; freq_div:inst|counter[16] ; freq_div:inst|counter[94]  ; clock      ; clock    ; None                        ; None                      ; 10.100 ns               ;
; N/A                                     ; 96.81 MHz ( period = 10.329 ns )                    ; freq_div:inst|counter[9]  ; freq_div:inst|counter[79]  ; clock      ; clock    ; None                        ; None                      ; 10.094 ns               ;
; N/A                                     ; 96.85 MHz ( period = 10.325 ns )                    ; freq_div:inst|counter[5]  ; freq_div:inst|counter[90]  ; clock      ; clock    ; None                        ; None                      ; 10.105 ns               ;
; N/A                                     ; 96.86 MHz ( period = 10.324 ns )                    ; freq_div:inst|counter[16] ; freq_div:inst|counter[98]  ; clock      ; clock    ; None                        ; None                      ; 10.093 ns               ;
; N/A                                     ; 96.94 MHz ( period = 10.316 ns )                    ; freq_div:inst|counter[2]  ; freq_div:inst|counter[85]  ; clock      ; clock    ; None                        ; None                      ; 10.103 ns               ;
; N/A                                     ; 97.00 MHz ( period = 10.309 ns )                    ; freq_div:inst|counter[15] ; freq_div:inst|counter[94]  ; clock      ; clock    ; None                        ; None                      ; 10.081 ns               ;
; N/A                                     ; 97.03 MHz ( period = 10.306 ns )                    ; freq_div:inst|counter[0]  ; freq_div:inst|counter[80]  ; clock      ; clock    ; None                        ; None                      ; 10.086 ns               ;
; N/A                                     ; 97.06 MHz ( period = 10.303 ns )                    ; freq_div:inst|counter[15] ; freq_div:inst|counter[98]  ; clock      ; clock    ; None                        ; None                      ; 10.074 ns               ;
; N/A                                     ; 97.07 MHz ( period = 10.302 ns )                    ; freq_div:inst|counter[2]  ; freq_div:inst|counter[83]  ; clock      ; clock    ; None                        ; None                      ; 10.082 ns               ;
; N/A                                     ; 97.18 MHz ( period = 10.290 ns )                    ; freq_div:inst|counter[6]  ; freq_div:inst|counter[90]  ; clock      ; clock    ; None                        ; None                      ; 10.070 ns               ;
; N/A                                     ; 97.29 MHz ( period = 10.279 ns )                    ; freq_div:inst|counter[0]  ; freq_div:inst|counter[82]  ; clock      ; clock    ; None                        ; None                      ; 10.059 ns               ;
; N/A                                     ; 97.30 MHz ( period = 10.278 ns )                    ; freq_div:inst|counter[20] ; freq_div:inst|counter[100] ; clock      ; clock    ; None                        ; None                      ; 10.049 ns               ;
; N/A                                     ; 97.31 MHz ( period = 10.276 ns )                    ; freq_div:inst|counter[10] ; freq_div:inst|counter[95]  ; clock      ; clock    ; None                        ; None                      ; 10.055 ns               ;
; N/A                                     ; 97.33 MHz ( period = 10.274 ns )                    ; freq_div:inst|counter[0]  ; freq_div:inst|counter[79]  ; clock      ; clock    ; None                        ; None                      ; 10.054 ns               ;
; N/A                                     ; 97.40 MHz ( period = 10.267 ns )                    ; freq_div:inst|counter[3]  ; freq_div:inst|counter[84]  ; clock      ; clock    ; None                        ; None                      ; 10.047 ns               ;
; N/A                                     ; 97.45 MHz ( period = 10.262 ns )                    ; freq_div:inst|counter[16] ; freq_div:inst|counter[93]  ; clock      ; clock    ; None                        ; None                      ; 10.032 ns               ;
; N/A                                     ; 97.45 MHz ( period = 10.262 ns )                    ; freq_div:inst|counter[11] ; freq_div:inst|counter[100] ; clock      ; clock    ; None                        ; None                      ; 10.040 ns               ;
; N/A                                     ; 97.48 MHz ( period = 10.258 ns )                    ; freq_div:inst|counter[13] ; freq_div:inst|counter[84]  ; clock      ; clock    ; None                        ; None                      ; 10.023 ns               ;
; N/A                                     ; 97.49 MHz ( period = 10.257 ns )                    ; freq_div:inst|counter[8]  ; freq_div:inst|counter[89]  ; clock      ; clock    ; None                        ; None                      ; 10.037 ns               ;
; N/A                                     ; 97.49 MHz ( period = 10.257 ns )                    ; freq_div:inst|counter[19] ; freq_div:inst|counter[94]  ; clock      ; clock    ; None                        ; None                      ; 10.029 ns               ;
; N/A                                     ; 97.55 MHz ( period = 10.251 ns )                    ; freq_div:inst|counter[19] ; freq_div:inst|counter[98]  ; clock      ; clock    ; None                        ; None                      ; 10.022 ns               ;
; N/A                                     ; 97.56 MHz ( period = 10.250 ns )                    ; freq_div:inst|counter[16] ; freq_div:inst|counter[99]  ; clock      ; clock    ; None                        ; None                      ; 10.019 ns               ;
; N/A                                     ; 97.60 MHz ( period = 10.246 ns )                    ; freq_div:inst|counter[7]  ; freq_div:inst|counter[74]  ; clock      ; clock    ; None                        ; None                      ; 10.012 ns               ;
; N/A                                     ; 97.60 MHz ( period = 10.246 ns )                    ; freq_div:inst|counter[3]  ; freq_div:inst|counter[88]  ; clock      ; clock    ; None                        ; None                      ; 10.033 ns               ;
; N/A                                     ; 97.60 MHz ( period = 10.246 ns )                    ; freq_div:inst|counter[5]  ; freq_div:inst|counter[96]  ; clock      ; clock    ; None                        ; None                      ; 10.032 ns               ;
; N/A                                     ; 97.64 MHz ( period = 10.242 ns )                    ; freq_div:inst|counter[3]  ; freq_div:inst|counter[86]  ; clock      ; clock    ; None                        ; None                      ; 10.029 ns               ;
; N/A                                     ; 97.65 MHz ( period = 10.241 ns )                    ; freq_div:inst|counter[15] ; freq_div:inst|counter[93]  ; clock      ; clock    ; None                        ; None                      ; 10.013 ns               ;
; N/A                                     ; 97.68 MHz ( period = 10.237 ns )                    ; freq_div:inst|counter[13] ; freq_div:inst|counter[88]  ; clock      ; clock    ; None                        ; None                      ; 10.009 ns               ;
; N/A                                     ; 97.70 MHz ( period = 10.235 ns )                    ; freq_div:inst|counter[8]  ; freq_div:inst|counter[92]  ; clock      ; clock    ; None                        ; None                      ; 10.015 ns               ;
; N/A                                     ; 97.72 MHz ( period = 10.233 ns )                    ; freq_div:inst|counter[13] ; freq_div:inst|counter[86]  ; clock      ; clock    ; None                        ; None                      ; 10.005 ns               ;
; N/A                                     ; 97.73 MHz ( period = 10.232 ns )                    ; freq_div:inst|counter[8]  ; freq_div:inst|counter[97]  ; clock      ; clock    ; None                        ; None                      ; 10.018 ns               ;
; N/A                                     ; 97.76 MHz ( period = 10.229 ns )                    ; freq_div:inst|counter[15] ; freq_div:inst|counter[99]  ; clock      ; clock    ; None                        ; None                      ; 10.000 ns               ;
; N/A                                     ; 97.85 MHz ( period = 10.220 ns )                    ; freq_div:inst|counter[1]  ; freq_div:inst|counter[81]  ; clock      ; clock    ; None                        ; None                      ; 10.000 ns               ;
; N/A                                     ; 97.92 MHz ( period = 10.212 ns )                    ; freq_div:inst|counter[3]  ; freq_div:inst|counter[87]  ; clock      ; clock    ; None                        ; None                      ; 9.999 ns                ;
; N/A                                     ; 97.92 MHz ( period = 10.212 ns )                    ; freq_div:inst|counter[20] ; freq_div:inst|counter[95]  ; clock      ; clock    ; None                        ; None                      ; 9.984 ns                ;
; Timing analysis restricted to 200 rows. ; To change the limit use Settings (Assignments menu) ;                           ;                            ;            ;          ;                             ;                           ;                         ;
+-----------------------------------------+-----------------------------------------------------+---------------------------+----------------------------+------------+----------+-----------------------------+---------------------------+-------------------------+


+---------------------------------------------------------------------------+
; tsu                                                                       ;
+-------+--------------+------------+-------+--------------------+----------+
; Slack ; Required tsu ; Actual tsu ; From  ; To                 ; To Clock ;
+-------+--------------+------------+-------+--------------------+----------+
; N/A   ; None         ; -2.654 ns  ; reset ; counter:inst1|c[1] ; clock    ;
; N/A   ; None         ; -2.654 ns  ; reset ; counter:inst1|c[2] ; clock    ;
; N/A   ; None         ; -2.654 ns  ; reset ; counter:inst1|c[3] ; clock    ;
; N/A   ; None         ; -2.933 ns  ; reset ; counter:inst1|c[0] ; clock    ;
+-------+--------------+------------+-------+--------------------+----------+


+------------------------------------------------------------------------------+
; tco                                                                          ;
+-------+--------------+------------+--------------------+--------+------------+
; Slack ; Required tco ; Actual tco ; From               ; To     ; From Clock ;
+-------+--------------+------------+--------------------+--------+------------+
; N/A   ; None         ; 12.293 ns  ; counter:inst1|c[1] ; out[2] ; clock      ;
; N/A   ; None         ; 12.215 ns  ; counter:inst1|c[2] ; out[2] ; clock      ;
; N/A   ; None         ; 12.064 ns  ; counter:inst1|c[1] ; out[1] ; clock      ;
; N/A   ; None         ; 12.061 ns  ; counter:inst1|c[1] ; out[3] ; clock      ;
; N/A   ; None         ; 12.017 ns  ; counter:inst1|c[2] ; out[1] ; clock      ;
; N/A   ; None         ; 12.012 ns  ; counter:inst1|c[0] ; out[2] ; clock      ;
; N/A   ; None         ; 12.012 ns  ; counter:inst1|c[2] ; out[3] ; clock      ;
; N/A   ; None         ; 11.979 ns  ; counter:inst1|c[2] ; out[0] ; clock      ;
; N/A   ; None         ; 11.945 ns  ; counter:inst1|c[1] ; out[0] ; clock      ;
; N/A   ; None         ; 11.777 ns  ; counter:inst1|c[0] ; out[1] ; clock      ;
; N/A   ; None         ; 11.772 ns  ; counter:inst1|c[0] ; out[3] ; clock      ;
; N/A   ; None         ; 11.745 ns  ; counter:inst1|c[0] ; out[0] ; clock      ;
; N/A   ; None         ; 11.742 ns  ; counter:inst1|c[1] ; out[6] ; clock      ;
; N/A   ; None         ; 11.734 ns  ; counter:inst1|c[1] ; out[4] ; clock      ;
; N/A   ; None         ; 11.727 ns  ; counter:inst1|c[1] ; out[5] ; clock      ;
; N/A   ; None         ; 11.691 ns  ; counter:inst1|c[2] ; out[6] ; clock      ;
; N/A   ; None         ; 11.683 ns  ; counter:inst1|c[2] ; out[4] ; clock      ;
; N/A   ; None         ; 11.676 ns  ; counter:inst1|c[2] ; out[5] ; clock      ;
; N/A   ; None         ; 11.653 ns  ; counter:inst1|c[3] ; out[2] ; clock      ;
; N/A   ; None         ; 11.452 ns  ; counter:inst1|c[0] ; out[6] ; clock      ;
; N/A   ; None         ; 11.443 ns  ; counter:inst1|c[0] ; out[4] ; clock      ;
; N/A   ; None         ; 11.442 ns  ; counter:inst1|c[0] ; out[5] ; clock      ;
; N/A   ; None         ; 11.421 ns  ; counter:inst1|c[3] ; out[1] ; clock      ;
; N/A   ; None         ; 11.416 ns  ; counter:inst1|c[3] ; out[3] ; clock      ;
; N/A   ; None         ; 11.389 ns  ; counter:inst1|c[3] ; out[0] ; clock      ;
; N/A   ; None         ; 11.096 ns  ; counter:inst1|c[3] ; out[6] ; clock      ;
; N/A   ; None         ; 11.087 ns  ; counter:inst1|c[3] ; out[4] ; clock      ;
; N/A   ; None         ; 11.083 ns  ; counter:inst1|c[3] ; out[5] ; clock      ;
+-------+--------------+------------+--------------------+--------+------------+


+---------------------------------------------------------------------------------+
; th                                                                              ;
+---------------+-------------+-----------+-------+--------------------+----------+
; Minimum Slack ; Required th ; Actual th ; From  ; To                 ; To Clock ;
+---------------+-------------+-----------+-------+--------------------+----------+
; N/A           ; None        ; 3.181 ns  ; reset ; counter:inst1|c[0] ; clock    ;
; N/A           ; None        ; 2.902 ns  ; reset ; counter:inst1|c[1] ; clock    ;
; N/A           ; None        ; 2.902 ns  ; reset ; counter:inst1|c[2] ; clock    ;
; N/A           ; None        ; 2.902 ns  ; reset ; counter:inst1|c[3] ; clock    ;
+---------------+-------------+-----------+-------+--------------------+----------+


+--------------------------+
; Timing Analyzer Messages ;
+--------------------------+
Info: *******************************************************************
Info: Running Quartus II Classic Timing Analyzer
    Info: Version 9.0 Build 132 02/25/2009 SJ Web Edition
    Info: Processing started: Wed Mar 24 16:40:20 2010
Info: Command: quartus_tan --read_settings_files=off --write_settings_files=off all -c all --timing_analysis_only
Warning: Found pins functioning as undefined clocks and/or memory enables
    Info: Assuming node "clock" is an undefined clock
Warning: Found 1 node(s) in clock paths which may be acting as ripple and/or gated clocks -- node(s) analyzed as buffer(s) resulting in clock skew
    Info: Detected ripple clock "freq_div:inst|freq2" as buffer
Info: Clock "clock" has Internal fmax of 86.93 MHz between source register "freq_div:inst|counter[7]" and destination register "freq_div:inst|counter[100]" (period= 11.504 ns)
    Info: + Longest register to register delay is 11.275 ns
        Info: 1: + IC(0.000 ns) + CELL(0.000 ns) = 0.000 ns; Loc. = LCFF_X23_Y18_N11; Fanout = 3; REG Node = 'freq_div:inst|counter[7]'
        Info: 2: + IC(1.194 ns) + CELL(0.495 ns) = 1.689 ns; Loc. = LCCOMB_X19_Y20_N26; Fanout = 2; COMB Node = 'freq_div:inst|Add0~15'
        Info: 3: + IC(0.000 ns) + CELL(0.080 ns) = 1.769 ns; Loc. = LCCOMB_X19_Y20_N28; Fanout = 2; COMB Node = 'freq_div:inst|Add0~17'
        Info: 4: + IC(0.000 ns) + CELL(0.161 ns) = 1.930 ns; Loc. = LCCOMB_X19_Y20_N30; Fanout = 2; COMB Node = 'freq_div:inst|Add0~19'
        Info: 5: + IC(0.000 ns) + CELL(0.080 ns) = 2.010 ns; Loc. = LCCOMB_X19_Y19_N0; Fanout = 2; COMB Node = 'freq_div:inst|Add0~21'
        Info: 6: + IC(0.000 ns) + CELL(0.080 ns) = 2.090 ns; Loc. = LCCOMB_X19_Y19_N2; Fanout = 2; COMB Node = 'freq_div:inst|Add0~23'
        Info: 7: + IC(0.000 ns) + CELL(0.080 ns) = 2.170 ns; Loc. = LCCOMB_X19_Y19_N4; Fanout = 2; COMB Node = 'freq_div:inst|Add0~25'
        Info: 8: + IC(0.000 ns) + CELL(0.080 ns) = 2.250 ns; Loc. = LCCOMB_X19_Y19_N6; Fanout = 2; COMB Node = 'freq_div:inst|Add0~27'
        Info: 9: + IC(0.000 ns) + CELL(0.080 ns) = 2.330 ns; Loc. = LCCOMB_X19_Y19_N8; Fanout = 2; COMB Node = 'freq_div:inst|Add0~29'
        Info: 10: + IC(0.000 ns) + CELL(0.080 ns) = 2.410 ns; Loc. = LCCOMB_X19_Y19_N10; Fanout = 2; COMB Node = 'freq_div:inst|Add0~31'
        Info: 11: + IC(0.000 ns) + CELL(0.080 ns) = 2.490 ns; Loc. = LCCOMB_X19_Y19_N12; Fanout = 2; COMB Node = 'freq_div:inst|Add0~33'
        Info: 12: + IC(0.000 ns) + CELL(0.174 ns) = 2.664 ns; Loc. = LCCOMB_X19_Y19_N14; Fanout = 2; COMB Node = 'freq_div:inst|Add0~35'
        Info: 13: + IC(0.000 ns) + CELL(0.080 ns) = 2.744 ns; Loc. = LCCOMB_X19_Y19_N16; Fanout = 2; COMB Node = 'freq_div:inst|Add0~37'
        Info: 14: + IC(0.000 ns) + CELL(0.080 ns) = 2.824 ns; Loc. = LCCOMB_X19_Y19_N18; Fanout = 2; COMB Node = 'freq_div:inst|Add0~39'
        Info: 15: + IC(0.000 ns) + CELL(0.080 ns) = 2.904 ns; Loc. = LCCOMB_X19_Y19_N20; Fanout = 2; COMB Node = 'freq_div:inst|Add0~41'
        Info: 16: + IC(0.000 ns) + CELL(0.080 ns) = 2.984 ns; Loc. = LCCOMB_X19_Y19_N22; Fanout = 2; COMB Node = 'freq_div:inst|Add0~43'
        Info: 17: + IC(0.000 ns) + CELL(0.080 ns) = 3.064 ns; Loc. = LCCOMB_X19_Y19_N24; Fanout = 2; COMB Node = 'freq_div:inst|Add0~45'
        Info: 18: + IC(0.000 ns) + CELL(0.080 ns) = 3.144 ns; Loc. = LCCOMB_X19_Y19_N26; Fanout = 2; COMB Node = 'freq_div:inst|Add0~47'
        Info: 19: + IC(0.000 ns) + CELL(0.080 ns) = 3.224 ns; Loc. = LCCOMB_X19_Y19_N28; Fanout = 2; COMB Node = 'freq_div:inst|Add0~49'
        Info: 20: + IC(0.000 ns) + CELL(0.161 ns) = 3.385 ns; Loc. = LCCOMB_X19_Y19_N30; Fanout = 2; COMB Node = 'freq_div:inst|Add0~51'
        Info: 21: + IC(0.000 ns) + CELL(0.080 ns) = 3.465 ns; Loc. = LCCOMB_X19_Y18_N0; Fanout = 2; COMB Node = 'freq_div:inst|Add0~53'
        Info: 22: + IC(0.000 ns) + CELL(0.080 ns) = 3.545 ns; Loc. = LCCOMB_X19_Y18_N2; Fanout = 2; COMB Node = 'freq_div:inst|Add0~55'
        Info: 23: + IC(0.000 ns) + CELL(0.080 ns) = 3.625 ns; Loc. = LCCOMB_X19_Y18_N4; Fanout = 2; COMB Node = 'freq_div:inst|Add0~57'
        Info: 24: + IC(0.000 ns) + CELL(0.080 ns) = 3.705 ns; Loc. = LCCOMB_X19_Y18_N6; Fanout = 2; COMB Node = 'freq_div:inst|Add0~59'
        Info: 25: + IC(0.000 ns) + CELL(0.080 ns) = 3.785 ns; Loc. = LCCOMB_X19_Y18_N8; Fanout = 2; COMB Node = 'freq_div:inst|Add0~61'
        Info: 26: + IC(0.000 ns) + CELL(0.080 ns) = 3.865 ns; Loc. = LCCOMB_X19_Y18_N10; Fanout = 2; COMB Node = 'freq_div:inst|Add0~63'
        Info: 27: + IC(0.000 ns) + CELL(0.080 ns) = 3.945 ns; Loc. = LCCOMB_X19_Y18_N12; Fanout = 2; COMB Node = 'freq_div:inst|Add0~65'
        Info: 28: + IC(0.000 ns) + CELL(0.174 ns) = 4.119 ns; Loc. = LCCOMB_X19_Y18_N14; Fanout = 2; COMB Node = 'freq_div:inst|Add0~67'
        Info: 29: + IC(0.000 ns) + CELL(0.080 ns) = 4.199 ns; Loc. = LCCOMB_X19_Y18_N16; Fanout = 2; COMB Node = 'freq_div:inst|Add0~69'
        Info: 30: + IC(0.000 ns) + CELL(0.080 ns) = 4.279 ns; Loc. = LCCOMB_X19_Y18_N18; Fanout = 2; COMB Node = 'freq_div:inst|Add0~71'
        Info: 31: + IC(0.000 ns) + CELL(0.080 ns) = 4.359 ns; Loc. = LCCOMB_X19_Y18_N20; Fanout = 2; COMB Node = 'freq_div:inst|Add0~73'
        Info: 32: + IC(0.000 ns) + CELL(0.080 ns) = 4.439 ns; Loc. = LCCOMB_X19_Y18_N22; Fanout = 2; COMB Node = 'freq_div:inst|Add0~75'
        Info: 33: + IC(0.000 ns) + CELL(0.080 ns) = 4.519 ns; Loc. = LCCOMB_X19_Y18_N24; Fanout = 2; COMB Node = 'freq_div:inst|Add0~77'
        Info: 34: + IC(0.000 ns) + CELL(0.080 ns) = 4.599 ns; Loc. = LCCOMB_X19_Y18_N26; Fanout = 2; COMB Node = 'freq_div:inst|Add0~79'
        Info: 35: + IC(0.000 ns) + CELL(0.080 ns) = 4.679 ns; Loc. = LCCOMB_X19_Y18_N28; Fanout = 2; COMB Node = 'freq_div:inst|Add0~81'
        Info: 36: + IC(0.000 ns) + CELL(0.161 ns) = 4.840 ns; Loc. = LCCOMB_X19_Y18_N30; Fanout = 2; COMB Node = 'freq_div:inst|Add0~83'
        Info: 37: + IC(0.000 ns) + CELL(0.080 ns) = 4.920 ns; Loc. = LCCOMB_X19_Y17_N0; Fanout = 2; COMB Node = 'freq_div:inst|Add0~85'
        Info: 38: + IC(0.000 ns) + CELL(0.080 ns) = 5.000 ns; Loc. = LCCOMB_X19_Y17_N2; Fanout = 2; COMB Node = 'freq_div:inst|Add0~87'
        Info: 39: + IC(0.000 ns) + CELL(0.080 ns) = 5.080 ns; Loc. = LCCOMB_X19_Y17_N4; Fanout = 2; COMB Node = 'freq_div:inst|Add0~89'
        Info: 40: + IC(0.000 ns) + CELL(0.080 ns) = 5.160 ns; Loc. = LCCOMB_X19_Y17_N6; Fanout = 2; COMB Node = 'freq_div:inst|Add0~91'
        Info: 41: + IC(0.000 ns) + CELL(0.080 ns) = 5.240 ns; Loc. = LCCOMB_X19_Y17_N8; Fanout = 2; COMB Node = 'freq_div:inst|Add0~93'
        Info: 42: + IC(0.000 ns) + CELL(0.080 ns) = 5.320 ns; Loc. = LCCOMB_X19_Y17_N10; Fanout = 2; COMB Node = 'freq_div:inst|Add0~95'
        Info: 43: + IC(0.000 ns) + CELL(0.080 ns) = 5.400 ns; Loc. = LCCOMB_X19_Y17_N12; Fanout = 2; COMB Node = 'freq_div:inst|Add0~97'
        Info: 44: + IC(0.000 ns) + CELL(0.174 ns) = 5.574 ns; Loc. = LCCOMB_X19_Y17_N14; Fanout = 2; COMB Node = 'freq_div:inst|Add0~99'
        Info: 45: + IC(0.000 ns) + CELL(0.080 ns) = 5.654 ns; Loc. = LCCOMB_X19_Y17_N16; Fanout = 2; COMB Node = 'freq_div:inst|Add0~101'
        Info: 46: + IC(0.000 ns) + CELL(0.080 ns) = 5.734 ns; Loc. = LCCOMB_X19_Y17_N18; Fanout = 2; COMB Node = 'freq_div:inst|Add0~103'
        Info: 47: + IC(0.000 ns) + CELL(0.080 ns) = 5.814 ns; Loc. = LCCOMB_X19_Y17_N20; Fanout = 2; COMB Node = 'freq_div:inst|Add0~105'
        Info: 48: + IC(0.000 ns) + CELL(0.080 ns) = 5.894 ns; Loc. = LCCOMB_X19_Y17_N22; Fanout = 2; COMB Node = 'freq_div:inst|Add0~107'
        Info: 49: + IC(0.000 ns) + CELL(0.080 ns) = 5.974 ns; Loc. = LCCOMB_X19_Y17_N24; Fanout = 2; COMB Node = 'freq_div:inst|Add0~109'
        Info: 50: + IC(0.000 ns) + CELL(0.080 ns) = 6.054 ns; Loc. = LCCOMB_X19_Y17_N26; Fanout = 2; COMB Node = 'freq_div:inst|Add0~111'
        Info: 51: + IC(0.000 ns) + CELL(0.080 ns) = 6.134 ns; Loc. = LCCOMB_X19_Y17_N28; Fanout = 2; COMB Node = 'freq_div:inst|Add0~113'
        Info: 52: + IC(0.000 ns) + CELL(0.161 ns) = 6.295 ns; Loc. = LCCOMB_X19_Y17_N30; Fanout = 2; COMB Node = 'freq_div:inst|Add0~115'
        Info: 53: + IC(0.000 ns) + CELL(0.080 ns) = 6.375 ns; Loc. = LCCOMB_X19_Y16_N0; Fanout = 2; COMB Node = 'freq_div:inst|Add0~117'
        Info: 54: + IC(0.000 ns) + CELL(0.080 ns) = 6.455 ns; Loc. = LCCOMB_X19_Y16_N2; Fanout = 2; COMB Node = 'freq_div:inst|Add0~119'
        Info: 55: + IC(0.000 ns) + CELL(0.080 ns) = 6.535 ns; Loc. = LCCOMB_X19_Y16_N4; Fanout = 2; COMB Node = 'freq_div:inst|Add0~121'
        Info: 56: + IC(0.000 ns) + CELL(0.080 ns) = 6.615 ns; Loc. = LCCOMB_X19_Y16_N6; Fanout = 2; COMB Node = 'freq_div:inst|Add0~123'
        Info: 57: + IC(0.000 ns) + CELL(0.080 ns) = 6.695 ns; Loc. = LCCOMB_X19_Y16_N8; Fanout = 2; COMB Node = 'freq_div:inst|Add0~125'
        Info: 58: + IC(0.000 ns) + CELL(0.080 ns) = 6.775 ns; Loc. = LCCOMB_X19_Y16_N10; Fanout = 2; COMB Node = 'freq_div:inst|Add0~127'
        Info: 59: + IC(0.000 ns) + CELL(0.080 ns) = 6.855 ns; Loc. = LCCOMB_X19_Y16_N12; Fanout = 2; COMB Node = 'freq_div:inst|Add0~129'
        Info: 60: + IC(0.000 ns) + CELL(0.174 ns) = 7.029 ns; Loc. = LCCOMB_X19_Y16_N14; Fanout = 2; COMB Node = 'freq_div:inst|Add0~131'
        Info: 61: + IC(0.000 ns) + CELL(0.080 ns) = 7.109 ns; Loc. = LCCOMB_X19_Y16_N16; Fanout = 2; COMB Node = 'freq_div:inst|Add0~133'
        Info: 62: + IC(0.000 ns) + CELL(0.080 ns) = 7.189 ns; Loc. = LCCOMB_X19_Y16_N18; Fanout = 2; COMB Node = 'freq_div:inst|Add0~135'
        Info: 63: + IC(0.000 ns) + CELL(0.080 ns) = 7.269 ns; Loc. = LCCOMB_X19_Y16_N20; Fanout = 2; COMB Node = 'freq_div:inst|Add0~137'
        Info: 64: + IC(0.000 ns) + CELL(0.080 ns) = 7.349 ns; Loc. = LCCOMB_X19_Y16_N22; Fanout = 2; COMB Node = 'freq_div:inst|Add0~139'
        Info: 65: + IC(0.000 ns) + CELL(0.080 ns) = 7.429 ns; Loc. = LCCOMB_X19_Y16_N24; Fanout = 2; COMB Node = 'freq_div:inst|Add0~141'
        Info: 66: + IC(0.000 ns) + CELL(0.080 ns) = 7.509 ns; Loc. = LCCOMB_X19_Y16_N26; Fanout = 2; COMB Node = 'freq_div:inst|Add0~143'
        Info: 67: + IC(0.000 ns) + CELL(0.080 ns) = 7.589 ns; Loc. = LCCOMB_X19_Y16_N28; Fanout = 2; COMB Node = 'freq_div:inst|Add0~145'
        Info: 68: + IC(0.000 ns) + CELL(0.161 ns) = 7.750 ns; Loc. = LCCOMB_X19_Y16_N30; Fanout = 2; COMB Node = 'freq_div:inst|Add0~147'
        Info: 69: + IC(0.000 ns) + CELL(0.080 ns) = 7.830 ns; Loc. = LCCOMB_X19_Y15_N0; Fanout = 2; COMB Node = 'freq_div:inst|Add0~149'
        Info: 70: + IC(0.000 ns) + CELL(0.080 ns) = 7.910 ns; Loc. = LCCOMB_X19_Y15_N2; Fanout = 2; COMB Node = 'freq_div:inst|Add0~151'
        Info: 71: + IC(0.000 ns) + CELL(0.080 ns) = 7.990 ns; Loc. = LCCOMB_X19_Y15_N4; Fanout = 2; COMB Node = 'freq_div:inst|Add0~153'
        Info: 72: + IC(0.000 ns) + CELL(0.080 ns) = 8.070 ns; Loc. = LCCOMB_X19_Y15_N6; Fanout = 2; COMB Node = 'freq_div:inst|Add0~155'
        Info: 73: + IC(0.000 ns) + CELL(0.080 ns) = 8.150 ns; Loc. = LCCOMB_X19_Y15_N8; Fanout = 2; COMB Node = 'freq_div:inst|Add0~157'
        Info: 74: + IC(0.000 ns) + CELL(0.080 ns) = 8.230 ns; Loc. = LCCOMB_X19_Y15_N10; Fanout = 2; COMB Node = 'freq_div:inst|Add0~159'
        Info: 75: + IC(0.000 ns) + CELL(0.080 ns) = 8.310 ns; Loc. = LCCOMB_X19_Y15_N12; Fanout = 2; COMB Node = 'freq_div:inst|Add0~161'
        Info: 76: + IC(0.000 ns) + CELL(0.174 ns) = 8.484 ns; Loc. = LCCOMB_X19_Y15_N14; Fanout = 2; COMB Node = 'freq_div:inst|Add0~163'
        Info: 77: + IC(0.000 ns) + CELL(0.080 ns) = 8.564 ns; Loc. = LCCOMB_X19_Y15_N16; Fanout = 2; COMB Node = 'freq_div:inst|Add0~165'
        Info: 78: + IC(0.000 ns) + CELL(0.080 ns) = 8.644 ns; Loc. = LCCOMB_X19_Y15_N18; Fanout = 2; COMB Node = 'freq_div:inst|Add0~167'
        Info: 79: + IC(0.000 ns) + CELL(0.080 ns) = 8.724 ns; Loc. = LCCOMB_X19_Y15_N20; Fanout = 2; COMB Node = 'freq_div:inst|Add0~169'
        Info: 80: + IC(0.000 ns) + CELL(0.080 ns) = 8.804 ns; Loc. = LCCOMB_X19_Y15_N22; Fanout = 2; COMB Node = 'freq_div:inst|Add0~171'
        Info: 81: + IC(0.000 ns) + CELL(0.080 ns) = 8.884 ns; Loc. = LCCOMB_X19_Y15_N24; Fanout = 2; COMB Node = 'freq_div:inst|Add0~173'
        Info: 82: + IC(0.000 ns) + CELL(0.080 ns) = 8.964 ns; Loc. = LCCOMB_X19_Y15_N26; Fanout = 2; COMB Node = 'freq_div:inst|Add0~175'
        Info: 83: + IC(0.000 ns) + CELL(0.080 ns) = 9.044 ns; Loc. = LCCOMB_X19_Y15_N28; Fanout = 2; COMB Node = 'freq_div:inst|Add0~177'
        Info: 84: + IC(0.000 ns) + CELL(0.161 ns) = 9.205 ns; Loc. = LCCOMB_X19_Y15_N30; Fanout = 2; COMB Node = 'freq_div:inst|Add0~179'
        Info: 85: + IC(0.000 ns) + CELL(0.080 ns) = 9.285 ns; Loc. = LCCOMB_X19_Y14_N0; Fanout = 2; COMB Node = 'freq_div:inst|Add0~181'
        Info: 86: + IC(0.000 ns) + CELL(0.080 ns) = 9.365 ns; Loc. = LCCOMB_X19_Y14_N2; Fanout = 2; COMB Node = 'freq_div:inst|Add0~183'
        Info: 87: + IC(0.000 ns) + CELL(0.080 ns) = 9.445 ns; Loc. = LCCOMB_X19_Y14_N4; Fanout = 2; COMB Node = 'freq_div:inst|Add0~185'
        Info: 88: + IC(0.000 ns) + CELL(0.080 ns) = 9.525 ns; Loc. = LCCOMB_X19_Y14_N6; Fanout = 2; COMB Node = 'freq_div:inst|Add0~187'
        Info: 89: + IC(0.000 ns) + CELL(0.080 ns) = 9.605 ns; Loc. = LCCOMB_X19_Y14_N8; Fanout = 2; COMB Node = 'freq_div:inst|Add0~189'
        Info: 90: + IC(0.000 ns) + CELL(0.080 ns) = 9.685 ns; Loc. = LCCOMB_X19_Y14_N10; Fanout = 2; COMB Node = 'freq_div:inst|Add0~191'
        Info: 91: + IC(0.000 ns) + CELL(0.080 ns) = 9.765 ns; Loc. = LCCOMB_X19_Y14_N12; Fanout = 2; COMB Node = 'freq_div:inst|Add0~193'
        Info: 92: + IC(0.000 ns) + CELL(0.174 ns) = 9.939 ns; Loc. = LCCOMB_X19_Y14_N14; Fanout = 2; COMB Node = 'freq_div:inst|Add0~195'
        Info: 93: + IC(0.000 ns) + CELL(0.080 ns) = 10.019 ns; Loc. = LCCOMB_X19_Y14_N16; Fanout = 2; COMB Node = 'freq_div:inst|Add0~197'
        Info: 94: + IC(0.000 ns) + CELL(0.080 ns) = 10.099 ns; Loc. = LCCOMB_X19_Y14_N18; Fanout = 1; COMB Node = 'freq_div:inst|Add0~199'
        Info: 95: + IC(0.000 ns) + CELL(0.458 ns) = 10.557 ns; Loc. = LCCOMB_X19_Y14_N20; Fanout = 1; COMB Node = 'freq_div:inst|Add0~200'
        Info: 96: + IC(0.303 ns) + CELL(0.319 ns) = 11.179 ns; Loc. = LCCOMB_X19_Y14_N30; Fanout = 1; COMB Node = 'freq_div:inst|counter~101'
        Info: 97: + IC(0.000 ns) + CELL(0.096 ns) = 11.275 ns; Loc. = LCFF_X19_Y14_N31; Fanout = 2; REG Node = 'freq_div:inst|counter[100]'
        Info: Total cell delay = 9.778 ns ( 86.72 % )
        Info: Total interconnect delay = 1.497 ns ( 13.28 % )
    Info: - Smallest clock skew is 0.010 ns
        Info: + Shortest clock path from clock "clock" to destination register is 2.860 ns
            Info: 1: + IC(0.000 ns) + CELL(1.026 ns) = 1.026 ns; Loc. = PIN_L1; Fanout = 2; CLK Node = 'clock'
            Info: 2: + IC(0.238 ns) + CELL(0.000 ns) = 1.264 ns; Loc. = CLKCTRL_G2; Fanout = 101; COMB Node = 'clock~clkctrl'
            Info: 3: + IC(0.994 ns) + CELL(0.602 ns) = 2.860 ns; Loc. = LCFF_X19_Y14_N31; Fanout = 2; REG Node = 'freq_div:inst|counter[100]'
            Info: Total cell delay = 1.628 ns ( 56.92 % )
            Info: Total interconnect delay = 1.232 ns ( 43.08 % )
        Info: - Longest clock path from clock "clock" to source register is 2.850 ns
            Info: 1: + IC(0.000 ns) + CELL(1.026 ns) = 1.026 ns; Loc. = PIN_L1; Fanout = 2; CLK Node = 'clock'
            Info: 2: + IC(0.238 ns) + CELL(0.000 ns) = 1.264 ns; Loc. = CLKCTRL_G2; Fanout = 101; COMB Node = 'clock~clkctrl'
            Info: 3: + IC(0.984 ns) + CELL(0.602 ns) = 2.850 ns; Loc. = LCFF_X23_Y18_N11; Fanout = 3; REG Node = 'freq_div:inst|counter[7]'
            Info: Total cell delay = 1.628 ns ( 57.12 % )
            Info: Total interconnect delay = 1.222 ns ( 42.88 % )
    Info: + Micro clock to output delay of source is 0.277 ns
    Info: + Micro setup delay of destination is -0.038 ns
Info: tsu for register "counter:inst1|c[1]" (data pin = "reset", clock pin = "clock") is -2.654 ns
    Info: + Longest pin to register delay is 4.248 ns
        Info: 1: + IC(0.000 ns) + CELL(1.026 ns) = 1.026 ns; Loc. = PIN_L22; Fanout = 5; PIN Node = 'reset'
        Info: 2: + IC(2.642 ns) + CELL(0.580 ns) = 4.248 ns; Loc. = LCFF_X1_Y20_N1; Fanout = 10; REG Node = 'counter:inst1|c[1]'
        Info: Total cell delay = 1.606 ns ( 37.81 % )
        Info: Total interconnect delay = 2.642 ns ( 62.19 % )
    Info: + Micro setup delay of destination is -0.038 ns
    Info: - Shortest clock path from clock "clock" to destination register is 6.864 ns
        Info: 1: + IC(0.000 ns) + CELL(1.026 ns) = 1.026 ns; Loc. = PIN_L1; Fanout = 2; CLK Node = 'clock'
        Info: 2: + IC(1.161 ns) + CELL(0.879 ns) = 3.066 ns; Loc. = LCFF_X19_Y13_N17; Fanout = 1; REG Node = 'freq_div:inst|freq2'
        Info: 3: + IC(2.226 ns) + CELL(0.000 ns) = 5.292 ns; Loc. = CLKCTRL_G13; Fanout = 4; COMB Node = 'freq_div:inst|freq2~clkctrl'
        Info: 4: + IC(0.970 ns) + CELL(0.602 ns) = 6.864 ns; Loc. = LCFF_X1_Y20_N1; Fanout = 10; REG Node = 'counter:inst1|c[1]'
        Info: Total cell delay = 2.507 ns ( 36.52 % )
        Info: Total interconnect delay = 4.357 ns ( 63.48 % )
Info: tco from clock "clock" to destination pin "out[2]" through register "counter:inst1|c[1]" is 12.293 ns
    Info: + Longest clock path from clock "clock" to source register is 6.864 ns
        Info: 1: + IC(0.000 ns) + CELL(1.026 ns) = 1.026 ns; Loc. = PIN_L1; Fanout = 2; CLK Node = 'clock'
        Info: 2: + IC(1.161 ns) + CELL(0.879 ns) = 3.066 ns; Loc. = LCFF_X19_Y13_N17; Fanout = 1; REG Node = 'freq_div:inst|freq2'
        Info: 3: + IC(2.226 ns) + CELL(0.000 ns) = 5.292 ns; Loc. = CLKCTRL_G13; Fanout = 4; COMB Node = 'freq_div:inst|freq2~clkctrl'
        Info: 4: + IC(0.970 ns) + CELL(0.602 ns) = 6.864 ns; Loc. = LCFF_X1_Y20_N1; Fanout = 10; REG Node = 'counter:inst1|c[1]'
        Info: Total cell delay = 2.507 ns ( 36.52 % )
        Info: Total interconnect delay = 4.357 ns ( 63.48 % )
    Info: + Micro clock to output delay of source is 0.277 ns
    Info: + Longest register to pin delay is 5.152 ns
        Info: 1: + IC(0.000 ns) + CELL(0.000 ns) = 0.000 ns; Loc. = LCFF_X1_Y20_N1; Fanout = 10; REG Node = 'counter:inst1|c[1]'
        Info: 2: + IC(0.670 ns) + CELL(0.542 ns) = 1.212 ns; Loc. = LCCOMB_X1_Y20_N8; Fanout = 1; COMB Node = 'sevenseg:inst2|WideOr4~0'
        Info: 3: + IC(1.100 ns) + CELL(2.840 ns) = 5.152 ns; Loc. = PIN_H2; Fanout = 0; PIN Node = 'out[2]'
        Info: Total cell delay = 3.382 ns ( 65.64 % )
        Info: Total interconnect delay = 1.770 ns ( 34.36 % )
Info: th for register "counter:inst1|c[0]" (data pin = "reset", clock pin = "clock") is 3.181 ns
    Info: + Longest clock path from clock "clock" to destination register is 6.864 ns
        Info: 1: + IC(0.000 ns) + CELL(1.026 ns) = 1.026 ns; Loc. = PIN_L1; Fanout = 2; CLK Node = 'clock'
        Info: 2: + IC(1.161 ns) + CELL(0.879 ns) = 3.066 ns; Loc. = LCFF_X19_Y13_N17; Fanout = 1; REG Node = 'freq_div:inst|freq2'
        Info: 3: + IC(2.226 ns) + CELL(0.000 ns) = 5.292 ns; Loc. = CLKCTRL_G13; Fanout = 4; COMB Node = 'freq_div:inst|freq2~clkctrl'
        Info: 4: + IC(0.970 ns) + CELL(0.602 ns) = 6.864 ns; Loc. = LCFF_X1_Y20_N31; Fanout = 11; REG Node = 'counter:inst1|c[0]'
        Info: Total cell delay = 2.507 ns ( 36.52 % )
        Info: Total interconnect delay = 4.357 ns ( 63.48 % )
    Info: + Micro hold delay of destination is 0.286 ns
    Info: - Shortest pin to register delay is 3.969 ns
        Info: 1: + IC(0.000 ns) + CELL(1.026 ns) = 1.026 ns; Loc. = PIN_L22; Fanout = 5; PIN Node = 'reset'
        Info: 2: + IC(2.669 ns) + CELL(0.178 ns) = 3.873 ns; Loc. = LCCOMB_X1_Y20_N30; Fanout = 1; COMB Node = 'counter:inst1|c~12'
        Info: 3: + IC(0.000 ns) + CELL(0.096 ns) = 3.969 ns; Loc. = LCFF_X1_Y20_N31; Fanout = 11; REG Node = 'counter:inst1|c[0]'
        Info: Total cell delay = 1.300 ns ( 32.75 % )
        Info: Total interconnect delay = 2.669 ns ( 67.25 % )
Info: Quartus II Classic Timing Analyzer was successful. 0 errors, 2 warnings
    Info: Peak virtual memory: 160 megabytes
    Info: Processing ended: Wed Mar 24 16:40:21 2010
    Info: Elapsed time: 00:00:01
    Info: Total CPU time (on all processors): 00:00:01


