#include "mbed.h"

DigitalOut led(LED1);

int main() {

 led=0;

 while (1) {

 led = !led;

 printf("Led is: %d\n",led.read());

 wait\_ms(500);

 }

}