{ "Info" "IQEXE_SEPARATOR" "" "Info: *******************************************************************" {  } {  } 3 0 "*******************************************************************" 0 0 "" 0 -1}
{ "Info" "IQEXE_START_BANNER_PRODUCT" "Classic Timing Analyzer Quartus II " "Info: Running Quartus II Classic Timing Analyzer" { { "Info" "IQEXE_START_BANNER_VERSION" "Version 9.0 Build 132 02/25/2009 SJ Web Edition " "Info: Version 9.0 Build 132 02/25/2009 SJ Web Edition" {  } {  } 0 0 "%1!s!" 0 0 "" 0 -1} { "Info" "IQEXE_START_BANNER_TIME" "Wed Mar 24 14:29:56 2010 " "Info: Processing started: Wed Mar 24 14:29:56 2010" {  } {  } 0 0 "Processing started: %1!s!" 0 0 "" 0 -1}  } {  } 4 0 "Running %2!s! %1!s!" 0 0 "" 0 -1}
{ "Info" "IQEXE_START_BANNER_COMMANDLINE" "quartus_tan --read_settings_files=off --write_settings_files=off ex1 -c ex1 --timing_analysis_only " "Info: Command: quartus_tan --read_settings_files=off --write_settings_files=off ex1 -c ex1 --timing_analysis_only" {  } {  } 0 0 "Command: %1!s!" 0 0 "" 0 -1}
{ "Info" "ITDB_FULL_TPD_RESULT" "D F 7.041 ns Longest " "Info: Longest tpd from source pin \"D\" to destination pin \"F\" is 7.041 ns" { { "Info" "ITDB_NODE_DELAY" "IC(0.000 ns) + CELL(1.006 ns) 1.006 ns D 1 PIN PIN_V12 1 " "Info: 1: + IC(0.000 ns) + CELL(1.006 ns) = 1.006 ns; Loc. = PIN_V12; Fanout = 1; PIN Node = 'D'" {  } { { "c:/altera/90/quartus/bin/TimingClosureFloorplan.fld" "" { Floorplan "c:/altera/90/quartus/bin/TimingClosureFloorplan.fld" "" "" { D } "NODE_NAME" } } { "ex1.bdf" "" { Schematic "E:/university/Thirdyear2/DigitalLab/MYWORK/exp7/quartus/xx/ex1.bdf" { { 272 184 352 288 "D" "" } } } }  } 0 0 "%4!d!: + %1!s! = %2!s!; Loc. = %6!s!; Fanout = %7!d!; %5!s! Node = '%3!s!'" 0 0 "" 0 -1} { "Info" "ITDB_NODE_DELAY" "IC(1.784 ns) + CELL(0.521 ns) 3.311 ns inst5 2 COMB LCCOMB_X49_Y14_N16 1 " "Info: 2: + IC(1.784 ns) + CELL(0.521 ns) = 3.311 ns; Loc. = LCCOMB_X49_Y14_N16; Fanout = 1; COMB Node = 'inst5'" {  } { { "c:/altera/90/quartus/bin/TimingClosureFloorplan.fld" "" { Floorplan "c:/altera/90/quartus/bin/TimingClosureFloorplan.fld" "" "2.305 ns" { D inst5 } "NODE_NAME" } } { "ex1.bdf" "" { Schematic "E:/university/Thirdyear2/DigitalLab/MYWORK/exp7/quartus/xx/ex1.bdf" { { 200 664 728 248 "inst5" "" } } } }  } 0 0 "%4!d!: + %1!s! = %2!s!; Loc. = %6!s!; Fanout = %7!d!; %5!s! Node = '%3!s!'" 0 0 "" 0 -1} { "Info" "ITDB_NODE_DELAY" "IC(0.890 ns) + CELL(2.840 ns) 7.041 ns F 3 PIN PIN_R20 0 " "Info: 3: + IC(0.890 ns) + CELL(2.840 ns) = 7.041 ns; Loc. = PIN_R20; Fanout = 0; PIN Node = 'F'" {  } { { "c:/altera/90/quartus/bin/TimingClosureFloorplan.fld" "" { Floorplan "c:/altera/90/quartus/bin/TimingClosureFloorplan.fld" "" "3.730 ns" { inst5 F } "NODE_NAME" } } { "ex1.bdf" "" { Schematic "E:/university/Thirdyear2/DigitalLab/MYWORK/exp7/quartus/xx/ex1.bdf" { { 216 760 936 232 "F" "" } } } }  } 0 0 "%4!d!: + %1!s! = %2!s!; Loc. = %6!s!; Fanout = %7!d!; %5!s! Node = '%3!s!'" 0 0 "" 0 -1} { "Info" "ITDB_TOTAL_CELL_DELAY" "4.367 ns ( 62.02 % ) " "Info: Total cell delay = 4.367 ns ( 62.02 % )" {  } {  } 0 0 "Total cell delay = %1!s! %2!s!" 0 0 "" 0 -1} { "Info" "ITDB_TOTAL_IC_DELAY" "2.674 ns ( 37.98 % ) " "Info: Total interconnect delay = 2.674 ns ( 37.98 % )" {  } {  } 0 0 "Total interconnect delay = %1!s! %2!s!" 0 0 "" 0 -1}  } { { "c:/altera/90/quartus/bin/TimingClosureFloorplan.fld" "" { Floorplan "c:/altera/90/quartus/bin/TimingClosureFloorplan.fld" "" "7.041 ns" { D inst5 F } "NODE_NAME" } } { "c:/altera/90/quartus/bin/Technology_Viewer.qrui" "" { "TechnologyMapViewer" "c:/altera/90/quartus/bin/Technology_Viewer.qrui" "7.041 ns" { D {} D~combout {} inst5 {} F {} } { 0.000ns 0.000ns 1.784ns 0.890ns } { 0.000ns 1.006ns 0.521ns 2.840ns } "" } }  } 0 0 "%4!s! tpd from source pin \"%1!s!\" to destination pin \"%2!s!\" is %3!s!" 0 0 "" 0 -1}
{ "Info" "IQEXE_ERROR_COUNT" "Classic Timing Analyzer 0 s 0 s Quartus II " "Info: Quartus II Classic Timing Analyzer was successful. 0 errors, 0 warnings" { { "Info" "IQEXE_END_PEAK_VSIZE_MEMORY" "159 " "Info: Peak virtual memory: 159 megabytes" {  } {  } 0 0 "Peak virtual memory: %1!s! megabytes" 0 0 "" 0 -1} { "Info" "IQEXE_END_BANNER_TIME" "Wed Mar 24 14:29:57 2010 " "Info: Processing ended: Wed Mar 24 14:29:57 2010" {  } {  } 0 0 "Processing ended: %1!s!" 0 0 "" 0 -1} { "Info" "IQEXE_ELAPSED_TIME" "00:00:01 " "Info: Elapsed time: 00:00:01" {  } {  } 0 0 "Elapsed time: %1!s!" 0 0 "" 0 -1} { "Info" "IQEXE_ELAPSED_CPU_TIME" "00:00:01 " "Info: Total CPU time (on all processors): 00:00:01" {  } {  } 0 0 "Total CPU time (on all processors): %1!s!" 0 0 "" 0 -1}  } {  } 0 0 "%6!s! %1!s! was successful. %2!d! error%3!s!, %4!d! warning%5!s!" 0 0 "" 0 -1}
