{ "Info" "IQEXE_SEPARATOR" "" "Info: *******************************************************************" {  } {  } 3 0 "*******************************************************************" 0 0 "" 0 -1}
{ "Info" "IQEXE_START_BANNER_PRODUCT" "Classic Timing Analyzer Quartus II " "Info: Running Quartus II Classic Timing Analyzer" { { "Info" "IQEXE_START_BANNER_VERSION" "Version 9.0 Build 132 02/25/2009 SJ Web Edition " "Info: Version 9.0 Build 132 02/25/2009 SJ Web Edition" {  } {  } 0 0 "%1!s!" 0 0 "" 0 -1} { "Info" "IQEXE_START_BANNER_TIME" "Tue Mar 30 21:24:05 2010 " "Info: Processing started: Tue Mar 30 21:24:05 2010" {  } {  } 0 0 "Processing started: %1!s!" 0 0 "" 0 -1}  } {  } 4 0 "Running %2!s! %1!s!" 0 0 "" 0 -1}
{ "Info" "IQEXE_START_BANNER_COMMANDLINE" "quartus_tan --read_settings_files=off --write_settings_files=off MYDecoder -c MYDecoder --timing_analysis_only " "Info: Command: quartus_tan --read_settings_files=off --write_settings_files=off MYDecoder -c MYDecoder --timing_analysis_only" {  } {  } 0 0 "Command: %1!s!" 0 0 "" 0 -1}
{ "Info" "ITDB_FULL_TPD_RESULT" "select\[1\] out\[3\] 12.956 ns Longest " "Info: Longest tpd from source pin \"select\[1\]\" to destination pin \"out\[3\]\" is 12.956 ns" { { "Info" "ITDB_NODE_DELAY" "IC(0.000 ns) + CELL(0.853 ns) 0.853 ns select\[1\] 1 PIN PIN_H10 4 " "Info: 1: + IC(0.000 ns) + CELL(0.853 ns) = 0.853 ns; Loc. = PIN_H10; Fanout = 4; PIN Node = 'select\[1\]'" {  } { { "c:/altera/90/quartus/bin/TimingClosureFloorplan.fld" "" { Floorplan "c:/altera/90/quartus/bin/TimingClosureFloorplan.fld" "" "" { select[1] } "NODE_NAME" } } { "MYDecoder.v" "" { Text "E:/university/Thirdyear2/DigitalLab/MYWORK/exp9/quartus/Decode2x4/MYDecoder.v" 3 -1 0 } }  } 0 0 "%4!d!: + %1!s! = %2!s!; Loc. = %6!s!; Fanout = %7!d!; %5!s! Node = '%3!s!'" 0 0 "" 0 -1} { "Info" "ITDB_NODE_DELAY" "IC(6.074 ns) + CELL(0.521 ns) 7.448 ns out~7 2 COMB LCCOMB_X10_Y21_N22 1 " "Info: 2: + IC(6.074 ns) + CELL(0.521 ns) = 7.448 ns; Loc. = LCCOMB_X10_Y21_N22; Fanout = 1; COMB Node = 'out~7'" {  } { { "c:/altera/90/quartus/bin/TimingClosureFloorplan.fld" "" { Floorplan "c:/altera/90/quartus/bin/TimingClosureFloorplan.fld" "" "6.595 ns" { select[1] out~7 } "NODE_NAME" } } { "MYDecoder.v" "" { Text "E:/university/Thirdyear2/DigitalLab/MYWORK/exp9/quartus/Decode2x4/MYDecoder.v" 4 -1 0 } }  } 0 0 "%4!d!: + %1!s! = %2!s!; Loc. = %6!s!; Fanout = %7!d!; %5!s! Node = '%3!s!'" 0 0 "" 0 -1} { "Info" "ITDB_NODE_DELAY" "IC(2.522 ns) + CELL(2.986 ns) 12.956 ns out\[3\] 3 PIN PIN_W7 0 " "Info: 3: + IC(2.522 ns) + CELL(2.986 ns) = 12.956 ns; Loc. = PIN_W7; Fanout = 0; PIN Node = 'out\[3\]'" {  } { { "c:/altera/90/quartus/bin/TimingClosureFloorplan.fld" "" { Floorplan "c:/altera/90/quartus/bin/TimingClosureFloorplan.fld" "" "5.508 ns" { out~7 out[3] } "NODE_NAME" } } { "MYDecoder.v" "" { Text "E:/university/Thirdyear2/DigitalLab/MYWORK/exp9/quartus/Decode2x4/MYDecoder.v" 4 -1 0 } }  } 0 0 "%4!d!: + %1!s! = %2!s!; Loc. = %6!s!; Fanout = %7!d!; %5!s! Node = '%3!s!'" 0 0 "" 0 -1} { "Info" "ITDB_TOTAL_CELL_DELAY" "4.360 ns ( 33.65 % ) " "Info: Total cell delay = 4.360 ns ( 33.65 % )" {  } {  } 0 0 "Total cell delay = %1!s! %2!s!" 0 0 "" 0 -1} { "Info" "ITDB_TOTAL_IC_DELAY" "8.596 ns ( 66.35 % ) " "Info: Total interconnect delay = 8.596 ns ( 66.35 % )" {  } {  } 0 0 "Total interconnect delay = %1!s! %2!s!" 0 0 "" 0 -1}  } { { "c:/altera/90/quartus/bin/TimingClosureFloorplan.fld" "" { Floorplan "c:/altera/90/quartus/bin/TimingClosureFloorplan.fld" "" "12.956 ns" { select[1] out~7 out[3] } "NODE_NAME" } } { "c:/altera/90/quartus/bin/Technology_Viewer.qrui" "" { "TechnologyMapViewer" "c:/altera/90/quartus/bin/Technology_Viewer.qrui" "12.956 ns" { select[1] {} select[1]~combout {} out~7 {} out[3] {} } { 0.000ns 0.000ns 6.074ns 2.522ns } { 0.000ns 0.853ns 0.521ns 2.986ns } "" } }  } 0 0 "%4!s! tpd from source pin \"%1!s!\" to destination pin \"%2!s!\" is %3!s!" 0 0 "" 0 -1}
{ "Info" "IQEXE_ERROR_COUNT" "Classic Timing Analyzer 0 s 0 s Quartus II " "Info: Quartus II Classic Timing Analyzer was successful. 0 errors, 0 warnings" { { "Info" "IQEXE_END_PEAK_VSIZE_MEMORY" "159 " "Info: Peak virtual memory: 159 megabytes" {  } {  } 0 0 "Peak virtual memory: %1!s! megabytes" 0 0 "" 0 -1} { "Info" "IQEXE_END_BANNER_TIME" "Tue Mar 30 21:24:07 2010 " "Info: Processing ended: Tue Mar 30 21:24:07 2010" {  } {  } 0 0 "Processing ended: %1!s!" 0 0 "" 0 -1} { "Info" "IQEXE_ELAPSED_TIME" "00:00:02 " "Info: Elapsed time: 00:00:02" {  } {  } 0 0 "Elapsed time: %1!s!" 0 0 "" 0 -1} { "Info" "IQEXE_ELAPSED_CPU_TIME" "00:00:02 " "Info: Total CPU time (on all processors): 00:00:02" {  } {  } 0 0 "Total CPU time (on all processors): %1!s!" 0 0 "" 0 -1}  } {  } 0 0 "%6!s! %1!s! was successful. %2!d! error%3!s!, %4!d! warning%5!s!" 0 0 "" 0 -1}
