{ "Info" "IQEXE_SEPARATOR" "" "Info: *******************************************************************" {  } {  } 3 0 "*******************************************************************" 0 0 "" 0 -1}
{ "Info" "IQEXE_START_BANNER_PRODUCT" "Classic Timing Analyzer Quartus II " "Info: Running Quartus II Classic Timing Analyzer" { { "Info" "IQEXE_START_BANNER_VERSION" "Version 9.0 Build 132 02/25/2009 SJ Web Edition " "Info: Version 9.0 Build 132 02/25/2009 SJ Web Edition" {  } {  } 0 0 "%1!s!" 0 0 "" 0 -1} { "Info" "IQEXE_START_BANNER_TIME" "Wed Mar 24 14:25:50 2010 " "Info: Processing started: Wed Mar 24 14:25:50 2010" {  } {  } 0 0 "Processing started: %1!s!" 0 0 "" 0 -1}  } {  } 4 0 "Running %2!s! %1!s!" 0 0 "" 0 -1}
{ "Info" "IQEXE_START_BANNER_COMMANDLINE" "quartus_tan --read_settings_files=off --write_settings_files=off ex1 -c ex1 --timing_analysis_only " "Info: Command: quartus_tan --read_settings_files=off --write_settings_files=off ex1 -c ex1 --timing_analysis_only" {  } {  } 0 0 "Command: %1!s!" 0 0 "" 0 -1}
{ "Info" "ITDB_FULL_TPD_RESULT" "C F 9.824 ns Longest " "Info: Longest tpd from source pin \"C\" to destination pin \"F\" is 9.824 ns" { { "Info" "ITDB_NODE_DELAY" "IC(0.000 ns) + CELL(0.873 ns) 0.873 ns C 1 PIN PIN_A3 1 " "Info: 1: + IC(0.000 ns) + CELL(0.873 ns) = 0.873 ns; Loc. = PIN_A3; Fanout = 1; PIN Node = 'C'" {  } { { "c:/altera/90/quartus/bin/TimingClosureFloorplan.fld" "" { Floorplan "c:/altera/90/quartus/bin/TimingClosureFloorplan.fld" "" "" { C } "NODE_NAME" } } { "ex1.bdf" "" { Schematic "E:/university/Thirdyear2/DigitalLab/MYWORK/exp7/quartus/xx/ex1.bdf" { { 224 184 352 240 "C" "" } } } }  } 0 0 "%4!d!: + %1!s! = %2!s!; Loc. = %6!s!; Fanout = %7!d!; %5!s! Node = '%3!s!'" 0 0 "" 0 -1} { "Info" "ITDB_NODE_DELAY" "IC(5.238 ns) + CELL(0.178 ns) 6.289 ns inst5 2 COMB LCCOMB_X1_Y24_N24 1 " "Info: 2: + IC(5.238 ns) + CELL(0.178 ns) = 6.289 ns; Loc. = LCCOMB_X1_Y24_N24; Fanout = 1; COMB Node = 'inst5'" {  } { { "c:/altera/90/quartus/bin/TimingClosureFloorplan.fld" "" { Floorplan "c:/altera/90/quartus/bin/TimingClosureFloorplan.fld" "" "5.416 ns" { C inst5 } "NODE_NAME" } } { "ex1.bdf" "" { Schematic "E:/university/Thirdyear2/DigitalLab/MYWORK/exp7/quartus/xx/ex1.bdf" { { 200 664 728 248 "inst5" "" } } } }  } 0 0 "%4!d!: + %1!s! = %2!s!; Loc. = %6!s!; Fanout = %7!d!; %5!s! Node = '%3!s!'" 0 0 "" 0 -1} { "Info" "ITDB_NODE_DELAY" "IC(0.520 ns) + CELL(3.015 ns) 9.824 ns F 3 PIN PIN_D5 0 " "Info: 3: + IC(0.520 ns) + CELL(3.015 ns) = 9.824 ns; Loc. = PIN_D5; Fanout = 0; PIN Node = 'F'" {  } { { "c:/altera/90/quartus/bin/TimingClosureFloorplan.fld" "" { Floorplan "c:/altera/90/quartus/bin/TimingClosureFloorplan.fld" "" "3.535 ns" { inst5 F } "NODE_NAME" } } { "ex1.bdf" "" { Schematic "E:/university/Thirdyear2/DigitalLab/MYWORK/exp7/quartus/xx/ex1.bdf" { { 216 760 936 232 "F" "" } } } }  } 0 0 "%4!d!: + %1!s! = %2!s!; Loc. = %6!s!; Fanout = %7!d!; %5!s! Node = '%3!s!'" 0 0 "" 0 -1} { "Info" "ITDB_TOTAL_CELL_DELAY" "4.066 ns ( 41.39 % ) " "Info: Total cell delay = 4.066 ns ( 41.39 % )" {  } {  } 0 0 "Total cell delay = %1!s! %2!s!" 0 0 "" 0 -1} { "Info" "ITDB_TOTAL_IC_DELAY" "5.758 ns ( 58.61 % ) " "Info: Total interconnect delay = 5.758 ns ( 58.61 % )" {  } {  } 0 0 "Total interconnect delay = %1!s! %2!s!" 0 0 "" 0 -1}  } { { "c:/altera/90/quartus/bin/TimingClosureFloorplan.fld" "" { Floorplan "c:/altera/90/quartus/bin/TimingClosureFloorplan.fld" "" "9.824 ns" { C inst5 F } "NODE_NAME" } } { "c:/altera/90/quartus/bin/Technology_Viewer.qrui" "" { "TechnologyMapViewer" "c:/altera/90/quartus/bin/Technology_Viewer.qrui" "9.824 ns" { C {} C~combout {} inst5 {} F {} } { 0.000ns 0.000ns 5.238ns 0.520ns } { 0.000ns 0.873ns 0.178ns 3.015ns } "" } }  } 0 0 "%4!s! tpd from source pin \"%1!s!\" to destination pin \"%2!s!\" is %3!s!" 0 0 "" 0 -1}
{ "Info" "IQEXE_ERROR_COUNT" "Classic Timing Analyzer 0 s 0 s Quartus II " "Info: Quartus II Classic Timing Analyzer was successful. 0 errors, 0 warnings" { { "Info" "IQEXE_END_PEAK_VSIZE_MEMORY" "159 " "Info: Peak virtual memory: 159 megabytes" {  } {  } 0 0 "Peak virtual memory: %1!s! megabytes" 0 0 "" 0 -1} { "Info" "IQEXE_END_BANNER_TIME" "Wed Mar 24 14:25:51 2010 " "Info: Processing ended: Wed Mar 24 14:25:51 2010" {  } {  } 0 0 "Processing ended: %1!s!" 0 0 "" 0 -1} { "Info" "IQEXE_ELAPSED_TIME" "00:00:01 " "Info: Elapsed time: 00:00:01" {  } {  } 0 0 "Elapsed time: %1!s!" 0 0 "" 0 -1} { "Info" "IQEXE_ELAPSED_CPU_TIME" "00:00:01 " "Info: Total CPU time (on all processors): 00:00:01" {  } {  } 0 0 "Total CPU time (on all processors): %1!s!" 0 0 "" 0 -1}  } {  } 0 0 "%6!s! %1!s! was successful. %2!d! error%3!s!, %4!d! warning%5!s!" 0 0 "" 0 -1}
